C310P to C310 FDM conversion to-do-list
- tuning clp to more neutral
- correcting lift and drag for 45°-flaps instead of 35°-flaps
- correcting lateral stability for missing ventral fin
- corrections for short nacelles

author: Ysop/FGFS
