
This model and all associated files are released under the GPL
This model was derived from the FlightGear c172p model.
Thanks to all that have contributed in any way to FlightGear project.

This is very much a work in progress.

Ercoupe
Model 415C, 75HP.

version beta

----

FDM:
- Elevators limited to +/- 13 degrees
- Remove rudder input and couple to aileron input
- Remove rudder steering and couple to aileron input
- Remove flaps
- Remove lift from speedbrakes.  Ercoupe windows will open in flight, the
  speedbrake will simulate this.

- Adjust weights based on www.ercoupe.net/ads/Log-94106.pdf
- Adjusted locations of all fdm items based on the type certificate and model
  measurements

- Added third fuel tank

- Stiffened nose gear by 50% based on model observations

- Adjusted drag due to speed brake deflection to yield a 10 mph drop in speed
  during stable flight at 100 mph.

----

TODO:
- There are some sound issues. The volume seems a bit to low in the inside
  views, but that's maybe only me. There is a "turboprop" sound in the inside
  views, but there are also some strange effects. I haven't looked into it more
  closely, but the volume seems to be depending on pitch and/or heading in some
  (rather rare) situations. I'll try to find out more.

