<?xml version="1.0"?>
<!-- 777 tutorial, (c) 2011 Thorsten Brehm -->

<PropertyList>
	<name>Introduction: Autopilot</name>
	<description>
Welcome aboard your 777 aircraft!

Require an aircraft type conversion? Need an upgrade from another aircraft type (or older fgfs sim)?
This tutorial quickly walks you through the features of the autopilot.
</description>

	<init>
		<set>
			<property>controls/electric/battery-switch</property>
			<value>1</value>
		</set>
		<set>
			<property>/autopilot/settings/target-speed-kt</property>
			<value>200</value>
		</set>
		<set>
			<property>/autopilot/settings/heading-bug-deg</property>
			<value>360</value>
		</set>
		<set>
			<property>/autopilot/settings/track-bug-deg</property>
			<value>360</value>
		</set>
		<set>
			<property>/autopilot/settings/counter-set-altitude-ft</property>
			<value>10000</value>
		</set>
		<set>
			<property>autopilot/locks/passive-mode</property>
			<value>1</value>
		</set>
	</init>

<step>
	<message>This entire panel is the MCP (mode control panel) ("autopilot").</message>
	<view>
	    <heading-offset-deg>327.9</heading-offset-deg>
	    <pitch-offset-deg>-13.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.6</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>63.4</field-of-view>
	</view>
	
	<marker>
	    <x-m>-1.8200</x-m>
	    <y-m>-0.0683</y-m>
	    <z-m>0.5733</z-m>
	    <scale>5.9500</scale>
	</marker>
</step>

<step>
	<message>The autopilot master switch. Must be enabled for any autopilot mode to work
	(cannot be engaged on ground).</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8292</x-m>
	    <y-m>-0.2592</y-m>
	    <z-m>0.5925</z-m>
	    <scale>1.0000</scale>
	</marker>
</step>

<step>
	<message>The PFD displays "A/P" whenever autopilot master switch is enabled.</message>
	<view>
	    <heading-offset-deg>357.2</heading-offset-deg>
	    <pitch-offset-deg>-19.4</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.5</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>39.9</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8508</x-m>
	    <y-m>-0.5459</y-m>
	    <z-m>0.4417</z-m>
	    <scale>1.6667</scale>
	</marker>
	<set>
		<property>instrumentation/afds/ap-modes/mode-annunciator</property>
		<value>A/P</value>
	</set>
</step>

<step>
	<message>The caution light comes on when the A/P disenganges (automatically or manually)
	and this A/P warning sound is audible.</message>
	<view>
	    <heading-offset-deg>357.2</heading-offset-deg>
	    <pitch-offset-deg>-19.4</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.5</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>39.9</field-of-view>
	</view>
	<marker>
	    <x-m>-1.7875</x-m>
	    <y-m>-0.4633</y-m>
	    <z-m>0.6042</z-m>
	    <scale>1.7167</scale>
	</marker>
	<set>
		<property>autopilot/locks/passive-mode</property>
		<value>0</value>
	</set>
	<set>
		<property>autopilot/locks/passive-mode</property>
		<value>1</value>
	</set>
</step>

<step>
	<message>The EICAS text display also shows "A/P disengage" when A/P is switched off.</message>
	<view>
	    <heading-offset-deg>326.4</heading-offset-deg>
	    <pitch-offset-deg>-21.6</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.5</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>39.9</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8566</x-m>
	    <y-m>0.0458</y-m>
	    <z-m>0.4542</z-m>
	    <scale>3.0667</scale>
	</marker>
	<set>
		<property>autopilot/locks/passive-mode</property>
		<value>0</value>
	</set>
	<set>
		<property>autopilot/locks/passive-mode</property>
		<value>1</value>
	</set>
</step>

<step>
	<message>Auto-thrust (A/T) arm switches for left/right engine. Keep both switches in sync (unless you have a single-engine failure).</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8333</x-m>
	    <y-m>-0.2267</y-m>
	    <z-m>0.5992</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Switches must be enganged, otherwise A/T has no effect for left or right engine.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8333</x-m>
	    <y-m>-0.2267</y-m>
	    <z-m>0.5992</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Arm auto-thrust for left and right engine now (click)!</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8333</x-m>
	    <y-m>-0.2267</y-m>
	    <z-m>0.5992</z-m>
	    <scale>1.1667</scale>
	</marker>
	<exit>
		<condition>
			<and>
				<property>/instrumentation/afds/inputs/at-armed</property>
				<property>/instrumentation/afds/inputs/at-armed[1]</property>
			</and>
		</condition>
	</exit>
</step>

<step>
	<message>Main switch to enable auto-thrust (cannot be engaged on ground).</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8158</x-m>
	    <y-m>-0.2267</y-m>
	    <z-m>0.5458</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Displays selected A/T target speed.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8158</x-m>
	    <y-m>-0.1725</y-m>
	    <z-m>0.5975</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>A/T speed selector. Select 230 knots now (use mouse scroll wheel)!</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8158</x-m>
	    <y-m>-0.1825</y-m>
	    <z-m>0.5583</z-m>
	    <scale>1.1667</scale>
	</marker>
	<exit>
		<condition>
			<equals>
				<property>/autopilot/settings/target-speed-kt</property>
				<value>230</value>
			</equals>
		</condition>
	</exit>
</step>

<step>
	<message>LNAV: lateral navigation (controls heading, follows route)</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8242</x-m>
	    <y-m>-0.1342</y-m>
	    <z-m>0.5942</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>VNAV (vertical navigation, changes altitude according to route)</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8242</x-m>
	    <y-m>-0.1342</y-m>
	    <z-m>0.5692</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>FLCH: flight level change. Climb/descend to selected target altitude - then hold altidude.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8200</x-m>
	    <y-m>-0.1342</y-m>
	    <z-m>0.5425</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Autopilot disengage. Panic bar. Hit button to disable all autopilot modes.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8167</x-m>
	    <y-m>-0.0976</y-m>
	    <z-m>0.5408</z-m>
	    <scale>2.3334</scale>
	</marker>
</step>

<step>
	<message>Selected autopilot target heading.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>-0.0526</y-m>
	    <z-m>0.5967</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Heading hold. Fly fixed heading. Press button to hold current heading.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>-0.0576</y-m>
	    <z-m>0.5433</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Inner switch: Target heading selector. Use left/middle mouse button to change target heading. Select heading 300 now (click)!</message> 
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>-0.0576</y-m>
	    <z-m>0.5708</z-m>
	    <scale>1.1667</scale>
	</marker>
	<exit>
		<condition>
			<equals>
				<property>/autopilot/settings/heading-bug-deg</property>
				<value>300</value>
			</equals>
		</condition>
	</exit>
</step>

<step>
	<message>Outer switch: bank limit selector. Use mouse scroll wheel to select maximum roll angle for autopilot. Select 25 degrees (max) now!</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>-0.0576</y-m>
	    <z-m>0.5708</z-m>
	    <scale>1.1667</scale>
	</marker>
	<exit>
		<condition>
			<equals>
				<property>instrumentation/afds/inputs/bank-limit-switch</property>
				<value>5</value>
			</equals>
		</condition>
	</exit>
</step>

<step>
	<message>Vertical target speed. Displays selected climb/sink rate in ft/min.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>0.0199</y-m>
	    <z-m>0.5958</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Vertical speed selector. Mouse scroll wheel changes target climb/sink rate.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>0.0124</y-m>
	    <z-m>0.5592</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>VS/FPA main switch. Press button to engange/disengage fixed climb/sink rate.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>0.0474</y-m>
	    <z-m>0.5442</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Target altitude display.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8250</x-m>
	    <y-m>0.0816</y-m>
	    <z-m>0.5958</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Altitude selector. Use mouse scroll wheel to change target altitude. Select 15000ft now (click)!</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>0.0816</y-m>
	    <z-m>0.5708</z-m>
	    <scale>1.1667</scale>
	</marker>
	<exit>
		<condition>
			<equals>
				<property>/autopilot/settings/counter-set-altitude-ft</property>
				<value>15000</value>
			</equals>
		</condition>
	</exit>
</step>

<step>
	<message>Altitude hold. Press button to engage vertical autopilot mode and hold current altitude.</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8142</x-m>
	    <y-m>0.0816</y-m>
	    <z-m>0.5442</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Localizer arm. Arms autopilot to engange on localizer as soon as signal is in range (uses NAV1 receiver).</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8250</x-m>
	    <y-m>0.1291</y-m>
	    <z-m>0.5658</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>Approach arm. Arms autopilot to engange on localizer and glide slope, as soon as signals are in range (NAV1).</message>
	<view>
	    <heading-offset-deg>358.3</heading-offset-deg>
	    <pitch-offset-deg>-16.8</pitch-offset-deg>
	    <roll-offset-deg>0.0</roll-offset-deg>
	    <x-offset-m>-0.2</x-offset-m>
	    <y-offset-m>0.8</y-offset-m>
	    <z-offset-m>-28.0381</z-offset-m>
	    <field-of-view>57.4</field-of-view>
	</view>
	<marker>
	    <x-m>-1.8250</x-m>
	    <y-m>0.1324</y-m>
	    <z-m>0.5392</z-m>
	    <scale>1.1667</scale>
	</marker>
</step>

<step>
	<message>That's it. More tutorials are available.</message>
</step>

<end></end>

</PropertyList>
