<PropertyList>
    <name>Taxi and Takeoff</name>
    <description>
We're now fully configured to begin our pushback and engine start. The passengers are on board and
you've just been given your clearance. As things start to happen very quickly from here on out, don't be
afraid to pause your sim between steps.
    </description>
    <audio-dir>Aircraft/747-400/tutorial</audio-dir>

	<step>
		<message>Turn TAXI LIGHT ON.</message>
		<exit>           
			<condition>                   
				<equals>
					<property>/controls/lighting/taxi-light</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Set flaps to 20.</message>
		<exit>
			<condition>    
				<equals>         
					<property>/controls/flight/flaps</property>
					<value>0.667</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>Release parking brake and taxi to runway 28R</message>
		<exit>
			<condition>
				<property>/controls/gear/brake-parking</property>
				<value>0</value>		
			</condition>
		</exit>
	</step>

	<step>
		<message>Taxi onto the runway and stop.</message>
	</step>

	<step>
		<message>Turn LANDING and STROBE lights ON.</message>
		<exit>
			<condition>   
				<and>
					<equals>    
						<property>/controls/lighting/landing-lights</property>
						<value>1</value>
					</equals>
					<equals> 
						<property>/controls/lighting/strobe</property>
						<value>1</value>
					</equals>
				</and>
			</condition>
		</exit>
	 </step>

	<step>
		<message>Enable Autothrottle.</message>
		<exit>
			<condition>            
				<or>
					<equals>    
						<property>/autopilot/locks/speed</property>
						<value>speed-with-throttle-ias</value>
					</equals>
					<equals> 
						<property>/autopilot/locks/speed</property>
						<value>speed-with-throttle-mach</value>
					</equals>
				</or>
			</condition>
		</exit>
	</step>

	<step>
	<message>Ensure that F/D is ON, runway heading (283) is set in HDG, IAS is set to V2, LNAV and VNAV are armed, and that altitude is 10,000.</message>
		<exit>
			<condition>  
				<equals>    
				<property>/autopilot/locks/passive-mode</property>
				<value>1</value>
				</equals>          
				<equals>    
				<property>/autopilot/settings/target/true-heading-deg</property>
				<value>283</value>
				</equals>
				<equals> 
				<property>/autopilot/settings/target-speed-kt</property>
				<value>185</value>
				</equals>
				<equals> 
				<property>/autopilot/settings/target-altitude-feet</property>
				<value>10000</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>At Rotate, slowly and smoothly pull back on the controls to become airborne.</message>
	</step>

	<step>
		<message>Adjust pitch and roll with the controls to center the flight director indictors.</message>
	</step>

	<step>
		<message>As soon as you're clear of the runway and your climb rate is at least 500 feet per minute, set the landing gear to UP.</message>
		<exit>
			<condition>             
				<equals> 
					<property>/controls/gear/gear-down</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
	</step>

</PropertyList>
