<?xml version="1.0"?>
<!-- 777 tutorial, (c) 2011 Thorsten Brehm -->

<PropertyList>
	<name>Checklist: Preflight</name>
	<description>Welcome aboard your 777-200ER aircraft!

Passengers are embarking and our lovely cabin crew is taking care of cabin preparations. You've filed a flight-plan and have just completed the briefing with your copilot. Now it's time to work preflight checklists and prepare the aircraft.

This preflight tutorial walks you through all the steps of preparing your aircraft.

Well, you could just press "s" for autostart and skip all this - but you're a real captain, aren't you?
	</description>

	<audio-dir>Aircraft/777-200/Tutorials</audio-dir>

	<init>
		<set>
			<property>controls/electric/battery-switch</property>
			<value>0</value>
		</set>
		<set>
			<property>/controls/flight/flaps</property>
			<value>0.0</value>
		</set>
		<set>
			<property>/controls/electric/APU-generator</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/electric/engine[0]/bus-tie</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/electric/engine[1]/bus-tie</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/engines/engine[0]/cutoff</property>
			<value>1</value>
		</set>
		<set>
			<property>controls/engines/engine[1]/cutoff</property>
			<value>1</value>
		</set>
		<set>
			<property>controls/electric/engine/generator</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/electric/engine[1]/generator</property>
			<value>0</value>
		</set>
		<set>
			<property>/sim/model/armrest</property>
			<value>0</value>
		</set>
		<set>
			<property>controls/flight/speedbrake-lever</property>
			<value>0</value>
		</set>
		<set>
			<property>instrumentation/transponder/mode-switch</property>
			<value>1</value>
		</set>
	</init>

	<step>
		<message>Ok, we start the preflight preparation with a quick outside walk-around. Nose gear, check.</message>
		<view>
			<view-number>1</view-number>
			<heading-offset-deg>182.1</heading-offset-deg>
			<pitch-offset-deg>-4.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.3</x-offset-m>
			<y-offset-m>-0.1</y-offset-m>
			<z-offset-m>-35.0</z-offset-m>
			<field-of-view>70</field-of-view>
		</view>
	</step>
	
	<step>
		<message>Left engine. Blades look ok...</message>	
		<view>
			<view-number>1</view-number>
			<heading-offset-deg>235.6</heading-offset-deg>
			<pitch-offset-deg>-12.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-20.0</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>Left main gear. Tyres OK. Brakes OK. Check.</message>	
		<view>
			<view-number>1</view-number>
			<heading-offset-deg>308.6</heading-offset-deg>
			<pitch-offset-deg>-15.2</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-18.0</z-offset-m>
		</view>
	</step>
	
	<step>
		<message>Right main gear. Tyres as good as new. Check.</message>	
		<view>
			<view-number>1</view-number>
			<heading-offset-deg>28.5</heading-offset-deg>
			<pitch-offset-deg>-14.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-18.0</z-offset-m>
		</view>
	</step>

	<step>
		<message>Right engine. No signs of leaking oil. Blades fine. Check.</message>	
		<view>
			<view-number>1</view-number>
			<heading-offset-deg>117.2</heading-offset-deg>
			<pitch-offset-deg>-13.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-18.0</z-offset-m>
		</view>
	</step>

	<step>
		<message>Back to the cockpit now...</message>	
		<view>
			<view-number>1</view-number>
			<heading-offset-deg>359.9</heading-offset-deg>
			<pitch-offset-deg>10.1</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.0</x-offset-m>
			<y-offset-m>0.0</y-offset-m>
			<z-offset-m>-100.0</z-offset-m>
		</view>
	</step>

	<step>
		<message>Back to the cockpit. Adjust seat. Fasten seatbelts...</message>
		<view>
			<view-number>0</view-number>
			<heading-offset-deg>360.0</heading-offset-deg>
			<pitch-offset-deg>0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.6</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
			<field-of-view>70</field-of-view>
		</view>
	</step>

	<step>
		<message>Lower arm rests (click)!</message>
		<exit>
			<condition>
				<property>/sim/model/armrest</property>
			</condition>
		</exit>
		<marker>
			<x-m>-0.8775</x-m>
			<y-m>0.2925</y-m>
			<z-m>0.3758</z-m>
			<scale>13.0000</scale>
		</marker>
		<view>
			<heading-offset-deg>255.9</heading-offset-deg>
			<pitch-offset-deg>-23.5</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.5</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
		</view>
	</step>

	<step>
		<message>Right, much better now!
		Select "Equipment -> Fuel and Payload". Check/adjust fuel, passengers, payload.</message>
		<view>
			<heading-offset-deg>360.0</heading-offset-deg>
			<pitch-offset-deg>0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.6</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
		</view>
	</step>

	<step>
		<message>Check: battery power ON</message>
		<exit>
			<condition>
				<property>controls/electric/battery-switch</property>
			</condition>
		</exit>
		<marker>
			<x-m>-1.1450</x-m>
			<y-m>-0.3492</y-m>
			<z-m>1.2375</z-m>
			<scale>3.0000</scale>
		</marker>
		<view>
			<heading-offset-deg>301.3</heading-offset-deg>
			<pitch-offset-deg>50.7</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.6</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
		</view>
	</step>

	<step>
		<message>Well done, the cockpit is powered now!</message>
		<view>
			<heading-offset-deg>338.2</heading-offset-deg>
			<pitch-offset-deg>-27.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.6</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
			<field-of-view>70.0</field-of-view>
		</view>
	</step>

	<step>
		<message>Check: auxiliary power unit (APU) ON</message>
		<exit>
			<condition>
				<property>/controls/electric/APU-generator</property>
			</condition>
		</exit>
		<marker>
			<x-m>-1.1683</x-m>
			<y-m>-0.2967</y-m>
			<z-m>1.2375</z-m>
			<scale>3.0000</scale>
		</marker>
		<view>
			<heading-offset-deg>301.3</heading-offset-deg>
			<pitch-offset-deg>50.7</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.6</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
		</view>
	</step>

	<step>
		<message>Check: left/right power-bus cross-feeds ON</message>
		<exit>
			<condition>
				<and>
					<property>controls/electric/engine[0]/bus-tie</property>
					<property>controls/electric/engine[1]/bus-tie</property>
				</and>
			</condition>
		</exit>
		<marker>
			<x-m>-1.2133</x-m>
			<y-m>-0.3033</y-m>
			<z-m>1.2300</z-m>
			<scale>7.0000</scale>
		</marker>
	</step>

	<step>
		<message>Check: transponder STANDBY (turn left = click middle-mouse button)</message>
		<marker>
			<x-m>-1.0842</x-m>
			<y-m>0.1750</y-m>
			<z-m>0.0150</z-m>
			<scale>3.0000</scale>
		</marker>
		<exit>
			<condition>
				<equals>
					<property>/instrumentation/transponder/mode-switch</property>
					<value>0</value>
				</equals>
			</condition>
		</exit>
		<view>
			<heading-offset-deg>269.4</heading-offset-deg>
			<pitch-offset-deg>-48.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.5</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
			<field-of-view>14.8</field-of-view>
		</view>
	</step>

	<step>
		<message>Check: altimeter (pressure) setting (turn left/right, use mouse buttons)</message>
		<marker>
			<x-m>-1.8033</x-m>
			<y-m>-0.1758</y-m>
			<z-m>0.2458</z-m>
			<scale>3.0000</scale>
		</marker>
		<exit>
			<condition>
				<greater-than>
					<property>/instrumentation/altimeter/indicated-altitude-ft</property>
					<value>-1</value>
				</greater-than>
			</condition>
		</exit>
		<view>
			<heading-offset-deg>312.0</heading-offset-deg>
			<pitch-offset-deg>-29.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.6</x-offset-m>
			<y-offset-m>0.8</y-offset-m>
			<z-offset-m>-22.8</z-offset-m>
			<field-of-view>70</field-of-view>
		</view>
	</step>
	
	<step>
		<message>Check: GPWS self-test (press and hold for 5 seconds)</message>
		<exit>
			<condition>
				<property>/instrumentation/mk-viii/inputs/discretes/self-test</property>
			</condition>
		</exit>
		<marker>
			<x-m>-1.8483</x-m>
			<y-m>0.1450</y-m>
			<z-m>0.4633</z-m>
			<scale>2.4333</scale>
		</marker>
	</step>

	<step>
		<message>Ok, preflight checklist complete! Continue with the "Pushback and Start-up" tutorial.</message>
	</step>

	<end>
	</end>

</PropertyList>
