<?xml version="1.0"?>
<!-- 777 tutorial, (c) 2011 Thorsten Brehm -->

<PropertyList>
	<name>Introduction: Cockpit</name>
	<description>Welcome aboard your 777-200ER aircraft!

Require an aircraft type conversion? Need an upgrade from another aircraft type (or older fgfs sim)?
This tutorial quickly walks you through the features of the cockpit in general.
</description>

<init>
	<set>
		<property>controls/electric/battery-switch</property>
		<value>1</value>
	</set>
</init>

<step>
	<message>Welcome to the 777 cockpit introduction. Let's have a look - from left to right...</message>
	<view>
		<heading-offset-deg>342.2</heading-offset-deg>
		<pitch-offset-deg>-36.6</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>120.0</field-of-view>
	</view>
</step>

<step>
	<message>Electronic flight bag (EFB) (airport map display).</message>
	<view>
		<heading-offset-deg>42.2</heading-offset-deg>
		<pitch-offset-deg>-38.1</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>57.4</field-of-view>
	</view>
	<marker>
		<x-m>-1.5084</x-m>
		<y-m>-1.0250</y-m>
		<z-m>0.3066</z-m>
		<scale>10.6834</scale>
	</marker>
</step>

<step>
	<message>Clock and timer. Use the timer to fly exact legs in a holding pattern.</message>
	<view>
		<heading-offset-deg>8.6</heading-offset-deg>
		<pitch-offset-deg>-23.0</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>38.6</field-of-view>
	</view>
	<marker>
		<x-m>-1.8450</x-m>
		<y-m>-0.6950</y-m>
		<z-m>0.4092</z-m>
		<scale>5.9500</scale>
	</marker>
</step>

<step>
	<message>The yoke. It'll rattle when you stall the plane.</message>
	<view>
		<heading-offset-deg>0.4</heading-offset-deg>
		<pitch-offset-deg>-44.1</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.5</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>56.1</field-of-view>
	</view>
	<set>
		<property>/instrumentation/weu/actuators/stick-shaker</property>
		<value>1</value>
	</set>
</step>

<step>
	<set>
		<property>/instrumentation/weu/actuators/stick-shaker</property>
		<value>0</value>
	</set>

	<message>The "primary flight display" (PFD) - most important cockpit instrument (separate tutorial available).</message>
	<view>
		<heading-offset-deg>358.9</heading-offset-deg>
		<pitch-offset-deg>-25.5</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>39.9</field-of-view>
	</view>
	<marker>
		<x-m>-1.8425</x-m>
		<y-m>-0.5383</y-m>
		<z-m>0.3975</z-m>
		<scale>7.9500</scale>
	</marker>
</step>

<step>
	<message>Master warning and caution lights for urgent alerts.
	You can click the lights to dismiss alerts and warning sounds (not now :) ).</message>
	<view>
		<heading-offset-deg>357.2</heading-offset-deg>
		<pitch-offset-deg>-19.4</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.5</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>39.9</field-of-view>
	</view>
	<marker>
		<x-m>-1.7875</x-m>
		<y-m>-0.4633</y-m>
		<z-m>0.6042</z-m>
		<scale>1.7167</scale>
	</marker>
	<set>
		<property>/instrumentation/weu/light/master-caution</property>
		<value>1</value>
	</set>
	<set>
		<property>/instrumentation/weu/light/master-warning</property>
		<value>1</value>
	</set>
	<set>
		<property>/instrumentation/weu/sound/stall-horn</property>
		<value>1</value>
	</set>
</step>

<step>
	<set>
		<property>/instrumentation/weu/light/master-caution</property>
		<value>0</value>
	</set>
	<set>
		<property>/instrumentation/weu/light/master-warning</property>
		<value>0</value>
	</set>
	<set>
		<property>/instrumentation/weu/sound/stall-horn</property>
		<value>0</value>
	</set>
	
	<message>The "navigation display" (ND). Displays traffic, route information and weather.</message>
	<view>
		<heading-offset-deg>342.6</heading-offset-deg>
		<pitch-offset-deg>-25.6</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>39.9</field-of-view>
	</view>
	<marker>
		<x-m>-1.8425</x-m>
		<y-m>-0.3117</y-m>
		<z-m>0.3950</z-m>
		<scale>7.9500</scale>
	</marker>
</step>

<step>
	<message>Standby attitude indicator (backup if PFD fails).</message>
	<view>
		<heading-offset-deg>331.7</heading-offset-deg>
		<pitch-offset-deg>-25.2</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>41.3</field-of-view>
	</view>
	<marker>
		<x-m>-1.8358</x-m>
		<y-m>-0.1550</y-m>
		<z-m>0.4633</z-m>
		<scale>3.9500</scale>
	</marker>
</step>

<step>
	<message>Standby airspeed indicator (backup if PFD fails).</message>
	<view>
		<heading-offset-deg>331.7</heading-offset-deg>
		<pitch-offset-deg>-25.2</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>41.3</field-of-view>
	</view>
	<marker>
		<x-m>-1.8358</x-m>
		<y-m>-0.1467</y-m>
		<z-m>0.3717</z-m>
		<scale>3.9500</scale>
	</marker>
</step>

<step>
	<message>Standby altimeter (backup if PFD fails).</message>
	<view>
		<heading-offset-deg>331.7</heading-offset-deg>
		<pitch-offset-deg>-25.2</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>41.3</field-of-view>
	</view>
	<marker>
		<x-m>-1.8200</x-m>
		<y-m>-0.1483</y-m>
		<z-m>0.2775</z-m>
		<scale>3.9500</scale>
	</marker>
</step>

<step>
	<message>Electronic flight instrument system (EFIS) control panel.</message>
	<view>
		<heading-offset-deg>2.8</heading-offset-deg>
		<pitch-offset-deg>-9.3</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.3</x-offset-m>
		<y-offset-m>0.7</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>37.7</field-of-view>
	</view>
	<marker>
		<x-m>-1.8292</x-m>
		<y-m>-0.3608</y-m>
		<z-m>0.5783</z-m>
		<scale>6.6834</scale>
	</marker>
</step>

<step>
	<message>The "mode control panel" (MCP) for autopilot (separate tutorial available).</message>
	<view>
		<heading-offset-deg>327.9</heading-offset-deg>
		<pitch-offset-deg>-13.8</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>63.4</field-of-view>
	</view>
	<marker>
		<x-m>-1.8200</x-m>
		<y-m>-0.0683</y-m>
		<z-m>0.5733</z-m>
		<scale>5.9500</scale>
	</marker>
	<set>
		<property>autopilot/locks/passive-mode</property>
		<value>0</value>
	</set>
	<set>
		<property>autopilot/locks/passive-mode</property>
		<value>1</value>
	</set>
</step>


<step>
	<message>The "Engine indication and crew alerting system" (EICAS).
	Shows engine status and general text messages/alerts.</message>
	<view>
		<heading-offset-deg>359.2</heading-offset-deg>
		<pitch-offset-deg>-26.5</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>0.1</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>53.7</field-of-view>
	</view>
	<marker>
		<x-m>-1.8442</x-m>
		<y-m>0.0192</y-m>
		<z-m>0.4033</z-m>
		<scale>9.9500</scale>
	</marker>
</step>

<step>
	<message>Panel for gear and ground proximity warning system (GPWS).</message>
	<view>
		<heading-offset-deg>359.2</heading-offset-deg>
		<pitch-offset-deg>-26.5</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>0.1</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>53.7</field-of-view>
	</view>
	<marker>
		<x-m>-1.8442</x-m>
		<y-m>0.1792</y-m>
		<z-m>0.3733</z-m>
		<scale>9.9500</scale>
	</marker>
	<set>
		<property>/instrumentation/mk-viii/inputs/discretes/self-test</property>
		<value>1</value>
	</set>
</step>

<step>
	<set>
		<property>/instrumentation/mk-viii/inputs/discretes/self-test</property>
		<value>0</value>
	</set>

	<message>Separate set of copilot's instruments.</message>
	<view>
		<heading-offset-deg>316.5</heading-offset-deg>
		<pitch-offset-deg>-22.5</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>0.0</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>91.2</field-of-view>
	</view>
	<marker>
		<x-m>-1.8059</x-m>
		<y-m>0.5083</y-m>
		<z-m>0.3792</z-m>
		<scale>13.9500</scale>
	</marker>
</step>

<step>
	<message>The "control display unit" (CDU). Flight computer for route/fuel/payload/takeoff/approach calculations.</message>
	<view>
		<heading-offset-deg>356.8</heading-offset-deg>
		<pitch-offset-deg>-59.2</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.2</x-offset-m>
		<y-offset-m>1.2</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>31.7</field-of-view>
	</view>
	<marker>
		<x-m>-1.7208</x-m>
		<y-m>-0.1525</y-m>
		<z-m>0.1642</z-m>
		<scale>9.4667</scale>
	</marker>
</step>

<step>
	<message>Secondary EICAS display (not implemented).</message>
	<view>
		<heading-offset-deg>359.4</heading-offset-deg>
		<pitch-offset-deg>-60.6</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>0.0</x-offset-m>
		<y-offset-m>1.3</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>31.7</field-of-view>
	</view>
	<marker>
		<x-m>-1.7208</x-m>
		<y-m>0.0208</y-m>
		<z-m>0.1642</z-m>
		<scale>9.4667</scale>
	</marker>
</step>

<step>
	<message>Pedestal with thrust, flap and trim controls.</message>
	<view>
		<heading-offset-deg>359.2</heading-offset-deg>
		<pitch-offset-deg>-60.1</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>0.0</x-offset-m>
		<y-offset-m>0.6</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>74.8</field-of-view>
	</view>
	<marker>
		<x-m>-1.3884</x-m>
		<y-m>0.0208</y-m>
		<z-m>0.1375</z-m>
		<scale>9.4667</scale>
	</marker>
</step>

<step>
	<message>Radio frequency controls (COM1+2, NAV1+2, ADF1+2).</message>
	<view>
		<heading-offset-deg>0.0</heading-offset-deg>
		<pitch-offset-deg>-71.5</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.1</x-offset-m>
		<y-offset-m>0.5</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>53.7</field-of-view>
	</view>
	<marker>
		<x-m>-1.2417</x-m>
		<y-m>-0.1008</y-m>
		<z-m>0.0183</z-m>
		<scale>4.0500</scale>
	</marker>
</step>

<step>
	<message>Transponder and TCAS panel. Controls identification signal and
	traffic collision alerting system.</message>
	<view>
		<heading-offset-deg>359.8</heading-offset-deg>
		<pitch-offset-deg>-88.2</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>0.1</x-offset-m>
		<y-offset-m>0.6</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>44.1</field-of-view>
	</view>
	<marker>
		<x-m>-1.0942</x-m>
		<y-m>0.1392</y-m>
		<z-m>0.0183</z-m>
		<scale>4.6834</scale>
	</marker>
	<set>
		<property>/instrumentation/tcas/inputs/mode</property>
		<value>1</value>
	</set>
	<set>
		<property>/instrumentation/tcas/inputs/self-test</property>
		<value>1</value>
	</set>
</step>

<step>
	<set>
		<property>/instrumentation/tcas/inputs/self-test</property>
		<value>0</value>
	</set>

	<message>Overhead panel for engine, tank/fuel and lighting controls.</message>
	<view>
		<heading-offset-deg>0.0</heading-offset-deg>
		<pitch-offset-deg>60.7</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.0</x-offset-m>
		<y-offset-m>0.9</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>120.0</field-of-view>
	</view>
	<marker>
		<x-m>-1.5084</x-m>
		<y-m>-1.0250</y-m>
		<z-m>0.3066</z-m>
		<scale>10.6834</scale>
	</marker>
</step>

<step>
	<message>Thanks, that's the quick cockpit overview. More tutorials on specific instruments available.</message>
	<view>
		<heading-offset-deg>342.2</heading-offset-deg>
		<pitch-offset-deg>-36.6</pitch-offset-deg>
		<roll-offset-deg>0.0</roll-offset-deg>
		<x-offset-m>-0.6</x-offset-m>
		<y-offset-m>0.8</y-offset-m>
		<z-offset-m>-22.8</z-offset-m>
		<field-of-view>120.0</field-of-view>
	</view>
</step>

<end></end>

</PropertyList>
