<?xml version="1.0"?>

<PropertyList>

<!-- Specific keys -->

   <key>
    <name>Ctrl-L</name>
    <desc>Unlock/Lock Prop Reversing</desc>
   </key>
   <key>
    <name>Ctrl-B</name>
    <desc>Engage/Disengage Prop Reverse</desc>
   </key>
   <key>
    <name>Ctrl-V</name>
    <desc>Pilot view</desc>
   </key>
   <key>
    <name>Ctrl-N</name>
    <desc>Copilot view</desc>
   </key>
   <key>
    <name>Ctrl-E</name>
    <desc>Engineer view</desc>
   </key>
   <key>
    <name>Ctrl-K</name>
    <desc>Cockpit observer view</desc>
   </key>
   <key>
    <name>Ctrl-O</name>
    <desc>Overhead panel view</desc>
   </key>
   <key>
    <name>Ctrl-J</name>
    <desc>Cockpit jumpseat view</desc>
   </key>
   <key>
    <name>=</name>
    <desc>Options menu</desc>
   </key>


<!-- FDM ops -->

<text>
Starting the Constellation's engines:

Engage the magnetos for the engines you wish to start by setting the
switches above the pilot seat to "Both". From the engineer's station,
locate the "MJB No. 1" panel to the upper left. Turn on the ship's
battery or ground cart battery. Turn on all generator switches. Below
that panel, find the "MJB No. 2" panel. Turn the "Engine Starter Select"
switch to the engine you want to start. Press "Start" and watch your
gauges for the engine to catch. Repeat for all 4 engines.

 ________________________Procedures_________________________
 Takeoff :
            flaps 1/4 2900 RPM,
            rotation at 130 kt (full load), 120 kt (landing load);
            retract gear below 165 k,
            retract flaps below 184 kt.
 Climb :
            48.0 inhg, 2600 RPM.
 Cruise :
            220 kt at 20000 ft, 197 kt at 25000 ft.
 Descent :
            max pitch.
 Approach :
            flaps 1/4 below 184 kt;
            gear below 165 kt, flaps 1/2 below 161 kt,
            flaps 3/4 below 154 kt, full flaps below 148 kt. 
 Landing :
            maintain 120 kt (landing load);
            touch down 110 kt (landing load), 100 kt (empty load).

<!-- Real data -->
 ________________________Limitations________________________
 Vne (never exceed) : 293 kt until 11000 ft; then - 11 kt / 2000 ft
 Vno (normal operation): 260 kt until 11000 ft, then - 9 kt / 2000 ft
 Vne at 20000 ft : 244 kt
 Vno at 20000 ft : 220 kt
 Vne at 25000 ft : 216 kt
 Vno at 25000 ft : 197 kt
 Vf (takeoff flaps 60%) : 184 kt
 Va (maneuvring) : 180 kt
 Vlo (landing gear operation) : 165 kt
 Vle (landing gear extension) : 165 kt
 Vf (approach flaps 66%) : 161 kt
 Vf (80%) : 153 kt
 Vf (landing flaps 100%) : 148 kt
   
 ceiling : 25000 ft
 cruise : 20000 ft
 range : 3600 NM

 take-off (2.75 minutes) at sea level : 54.5 inhg 2900 rpm
 take-off (2.75 minutes) at 4500 ft : 52.5 inhg 2900 rpm
 maximum at sea level : 48.0 inhg 2600 rpm
 maximum at 5300 ft : 46.0 inhg 2600 rpm
 maximum at 10800 ft : 47.5 inhg 2600 rpm
 maximum at 16000 ft : 46.0 inhg 2600 rpm

 max take-off : 120000 lb
 max landing : 98500 lb
</text>

</PropertyList>
