<?xml version="1.0" encoding="UTF-8"?>
<!--###################################################################################
		Lake of Constance Hangar :: M.Kraus
		Boeing 707 for Flightgear Septemper 2013
		This file is licenced under the terms of the GNU General Public Licence V2 or later
		###################################################################################
-->
<PropertyList>
	<name>Engines: Start-up [english]</name>
	<description>Startup engines with external power unit.</description>

	<init>
		<set>
			<property>/sim/current-view/view-number</property>
			<value>0</value>
		</set>
		<set>
			<property>/controls/gear/brake-parking</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/flight/flaps</property>
			<value>0.0</value>
		</set>
		<set>
			<property>/b707/generator/gen-bus-tie[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-breaker[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-control[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-drive[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-bus-tie[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-breaker[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-control[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-drive[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-bus-tie[2]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-breaker[2]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-control[2]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-drive[2]</property>
			<value>0</value>
		</set>
		<set>
			<property>/controls/electric/engine[2]/generator</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-bus-tie[3]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-breaker[3]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-control[3]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/generator/gen-drive[3]</property>
			<value>0</value>
		</set>
		<set>
			<property>/controls/engines/engine[0]/cutoff</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/engines/engine[1]/cutoff</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/engines/engine[2]/cutoff</property>
			<value>1</value>
		</set>
		<set>
			<property>/controls/engines/engine[3]/cutoff</property>
			<value>1</value>
		</set>
		<set>
			<property>/b707/fuel/valves/valve-pos[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/valve-pos[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/valve-pos[2]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/valve-pos[3]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/valve-pos[4]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/valve-pos[5]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[3]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[4]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[5]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[6]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[7]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[8]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/boost-pump[9]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/fuel-shutoff[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/fuel-shutoff[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/fuel-shutoff[2]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/fuel/valves/fuel-shutoff[3]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/load-volt-selector</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/external-power-connected</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/battery-switch</property>
			<value>0</value>
		</set>		
		<set>
			<property>/b707/hydraulic/rudder</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/system</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/brake-valve</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/ac-aux-pump[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/ac-aux-pump[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/hyd-fluid-shutoff-cover[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/hyd-fluid-shutoff-cover[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/hyd-fluid-shutoff[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/hyd-fluid-shutoff[1]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/hyd-fluid-pump[0]</property>
			<value>0</value>
		</set>
		<set>
			<property>/b707/hydraulic/hyd-fluid-pump[1]</property>
			<value>0</value>
		</set>

	</init>

	<step>
		<message>
			Connect to External Power Unit.
			In main menu B707/External Power Unit
		</message>
		<view>
				<heading-offset-deg>240.8</heading-offset-deg>
				<pitch-offset-deg>4.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>49.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.5636</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.3967</z-m>
				<scale>1.6612</scale>
		</marker>

		<exit>
			<condition>
				<property>/b707/external-power-connected</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			The External Power Unit was plugged in.
		</message>
		<view>
		    <view-number>1</view-number>
				<heading-offset-deg>195.9</heading-offset-deg>
				<pitch-offset-deg>-3.7</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>25.0</x-offset-m>
				<y-offset-m>2.0</y-offset-m>
				<z-offset-m>-45.0</z-offset-m>
				<field-of-view>21.6</field-of-view>
		</view>
		<exit>
			<condition>
				<property>/b707/external-power-connected</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Switch on the battery.
		</message>
		<view>
				<heading-offset-deg>235.4</heading-offset-deg>
				<pitch-offset-deg>7.9</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>51.5</field-of-view>
		</view>

		<marker>
				<x-m>-17.5901</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.4587</z-m>
				<scale>2.3719</scale>
		</marker>

		<error>
			<message>Open the cover and switch on the battery.</message>
			<condition>
				<not><property>/b707/battery-switch</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/battery-switch</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			SELECTOR LOAD &amp; VOLTS turn to BUS-TIE.
		</message>
		<view>
				<heading-offset-deg>234.0</heading-offset-deg>
				<pitch-offset-deg>14.4</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>14.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.5554</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.4628</z-m>
				<scale>3.0000</scale>
		</marker>
		<error>
			<message>Use only BUS TIE for the moment.</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/load-volt-selector</property>
						<value>1</value>
					</less-than>
					<greater-than>
						<property>/b707/load-volt-selector</property>
						<value>1</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/load-volt-selector</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			ESSENTIAL POWER turn to EXT PWR.
		</message>
		<view>
				<heading-offset-deg>238.1</heading-offset-deg>
				<pitch-offset-deg>7.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>14.5</field-of-view>
		</view>

		<marker>
				<x-m>-17.5620</x-m>
				<y-m>0.6000</y-m>
				<z-m>1.3686</z-m>
				<scale>1.3967</scale>
		</marker>
		<error>
			<message>turn to EXT PWR.</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ess-power-switch</property>
						<value>5</value>
					</less-than>
					<greater-than>
						<property>/b707/ess-power-switch</property>
						<value>5</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ess-power-switch</property>
					<value>5</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			SELECTOR AC PARALLELING set to External Power.
			The AC source will be synchronized to 400Hz.
		</message>
		<view>
				<heading-offset-deg>241.4</heading-offset-deg>
				<pitch-offset-deg>3.4</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>15.9</field-of-view>
		</view>

		<marker>
				<x-m>-17.6165</x-m>
				<y-m>0.6000</y-m>
				<z-m>1.2488</z-m>
				<scale>1.3967</scale>
		</marker>
		<error>
			<message>select External Power.</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ac/ac-para-select</property>
						<value>6</value>
					</less-than>
					<greater-than>
						<property>/b707/ac/ac-para-select</property>
						<value>6</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ac/ac-para-select</property>
					<value>6</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			AUXILLIARY PUMPS on.
			Hydraulic pressure for rudder, gear and system support.
		</message>
		<view>
				<heading-offset-deg>230.5</heading-offset-deg>
				<pitch-offset-deg>-17.6</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>17.7</field-of-view>
		</view>

		<marker>
				<x-m>-17.4422</x-m>
				<y-m>0.7289</y-m>
				<z-m>0.7942</z-m>
				<scale>1.4959</scale>
		</marker>

		<error>
			<message>Switch both to on and wait until 3000 PSI RUD HYD PRESS.</message>
			<condition>
				<or>
					<not><property>/b707/hydraulic/ac-aux-pump[0]</property></not>
					<not><property>/b707/hydraulic/ac-aux-pump[1]</property></not>
					<less-than>
						<property>/b707/hydraulic/rudder</property>
						<value>2900</value>
					</less-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
			 <and>
				<property>/b707/hydraulic/ac-aux-pump[0]</property>
				<property>/b707/hydraulic/ac-aux-pump[1]</property>
				<greater-than>
					<property>/b707/hydraulic/rudder</property>
					<value>2900</value>
				</greater-than>
			 </and>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			INTERCONNECT VALVE on.
			AC AUXILLIARY PUMPS support system.
		</message>
		<view>
				<heading-offset-deg>230.5</heading-offset-deg>
				<pitch-offset-deg>-17.6</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>17.7</field-of-view>
		</view>

		<marker>
				<x-m>-17.4066</x-m>
				<y-m>0.7289</y-m>
				<z-m>0.7942</z-m>
				<scale>1.4959</scale>
		</marker>
		
		<error>
			<message>Switch down this knob</message>
			<condition>
				<not>
					<equals>
						<property>b707/hydraulic/brake-valve</property>
						<value>2</value>
					</equals>
				</not>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>b707/hydraulic/brake-valve</property>
					<value>2</value>
				</equals>
			</condition>
		</exit>
	</step>		
	
	<step>
		<message>
			HYD FLUID SHUTOFFs on.
		</message>
		<view>
				<heading-offset-deg>230.5</heading-offset-deg>
				<pitch-offset-deg>-17.6</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>17.7</field-of-view>
		</view>

		<marker>
				<x-m>-17.3207</x-m>
				<y-m>0.7289</y-m>
				<z-m>0.7942</z-m>
				<scale>2.7686</scale>
		</marker>

		<error>
			<message>Open covers and switch on the knobs.</message>
			<condition>
				<or>
					<not><property>/b707/hydraulic/hyd-fluid-shutoff[0]</property></not>
					<not><property>/b707/hydraulic/hyd-fluid-shutoff[1]</property></not>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<and>
					<property>/b707/hydraulic/hyd-fluid-shutoff[0]</property>
					<property>/b707/hydraulic/hyd-fluid-shutoff[1]</property>
				</and>
			</condition>
		</exit>
	</step>	
	
	<step>
		<message>
			ENGINE PUMPS on.
			Hydraulic support for all the residual systems.
		</message>
		<view>
				<heading-offset-deg>230.5</heading-offset-deg>
				<pitch-offset-deg>-17.6</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>17.7</field-of-view>
		</view>

		<marker>
				<x-m>-17.3744</x-m>
				<y-m>0.7289</y-m>
				<z-m>0.7918</z-m>
				<scale>1.5124</scale>
		</marker>

		<error>
			<message>Switch both to on and wait until 2200 PSI HYD SYS PRESS.</message>
			<condition>
				<or>
					<not><property>/b707/hydraulic/hyd-fluid-pump[0]</property></not>
					<not><property>/b707/hydraulic/hyd-fluid-pump[1]</property></not>					
					<less-than>
						<property>/b707/hydraulic/system</property>
						<value>2000</value>
					</less-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<and>
					<property>/b707/hydraulic/hyd-fluid-pump[0]</property>
					<property>/b707/hydraulic/hyd-fluid-pump[1]</property>
					<greater-than>
						<property>/b707/hydraulic/system</property>
						<value>2000</value>
					</greater-than>
				</and>
			</condition>
		</exit>
	</step>	
	
	<step>
		<message>
			Connect External Power Unit to the SYNC BUS.
		</message>
		<view>
				<heading-offset-deg>237.8</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>15.9</field-of-view>
		</view>

		<marker>
				<x-m>-17.5785</x-m>
				<y-m>0.6000</y-m>
				<z-m>1.4091</z-m>
				<scale>1.4959</scale>
		</marker>
		<error>
			<message>
				Switch to ON.
			</message>
			<condition>
				<not><property>/b707/ground-connect</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/ground-connect</property>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Connect the GEN - DRIVES.
			Open the red cover and switch on the drives. 
			Close cover then.
		</message>
		<view>
				<heading-offset-deg>241.8</heading-offset-deg>
				<pitch-offset-deg>14.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>22.8</field-of-view>
		</view>

		<marker>
				<x-m>-17.8587</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.4603</z-m>
				<scale>1.6612</scale>
		</marker>
		<error>
			<message>
				Connect all GEN - DRIVES and close then all the covers.
				Reconnect in flight is impossible.
			</message>
			<condition>
				<not><property>/b707/generator/gen-drive[0]</property></not>
				<not><property>/b707/generator/gen-drive[1]</property></not>
				<not><property>/b707/generator/gen-drive[2]</property></not>
				<not><property>/b707/generator/gen-drive[3]</property></not>
				<property>/b707/generator/gen-drive-cover[0]</property>
				<property>/b707/generator/gen-drive-cover[1]</property>
				<property>/b707/generator/gen-drive-cover[2]</property>
				<property>/b707/generator/gen-drive-cover[3]</property>
			</condition>
		</error>		
		<exit>
			<condition>
				<property>/b707/generator/gen-drive[0]</property>
				<property>/b707/generator/gen-drive[1]</property>
				<property>/b707/generator/gen-drive[2]</property>
				<property>/b707/generator/gen-drive[3]</property>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			BUS-TIE-BREAKER
			Open all covers and set the BUS-TIE-BREAKER to sync bus.
			Close cover then.
		</message>
		<view>
				<heading-offset-deg>244.9</heading-offset-deg>
				<pitch-offset-deg>9.7</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>16.7</field-of-view>
		</view>

		<marker>
				<x-m>-17.8653</x-m>
				<y-m>0.5992</y-m>
				<z-m>1.3669</z-m>
				<scale>1.6628</scale>
		</marker>
		<error>
			<message>
				Switch on all the buses and close the covers!
			</message>
			<condition>
				<not><property>/b707/generator/gen-bus-tie[0]</property></not>
				<not><property>/b707/generator/gen-bus-tie[1]</property></not>
				<not><property>/b707/generator/gen-bus-tie[2]</property></not>
				<not><property>/b707/generator/gen-bus-tie[3]</property></not>
				<property>/b707/generator/gen-bus-tie-cover[0]</property>
				<property>/b707/generator/gen-bus-tie-cover[1]</property>
				<property>/b707/generator/gen-bus-tie-cover[2]</property>
				<property>/b707/generator/gen-bus-tie-cover[3]</property>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/generator/gen-bus-tie[0]</property>
				<property>/b707/generator/gen-bus-tie[1]</property>
				<property>/b707/generator/gen-bus-tie[2]</property>
				<property>/b707/generator/gen-bus-tie[3]</property>
			</condition>
		</exit>
	</step>	
	
	<step>
		<message>
			GEN - CONTROL
			Open all covers and switch on the generator controllers.
			Close covers then.
		</message>
		<view>
				<heading-offset-deg>246.5</heading-offset-deg>
				<pitch-offset-deg>8.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>17.8</field-of-view>
		</view>

		<marker>
				<x-m>-17.8620</x-m>
				<y-m>0.6661</y-m>
				<z-m>1.2860</z-m>
				<scale>1.8430</scale>
		</marker>
		<error>
			<message>
				Switch on all controllers and close the covers!
			</message>
			<condition>
				<not><property>/b707/generator/gen-control[0]</property></not>
				<not><property>/b707/generator/gen-control[1]</property></not>
				<not><property>/b707/generator/gen-control[2]</property></not>
				<not><property>/b707/generator/gen-control[3]</property></not>
				<property>/b707/generator/gen-control-cover[0]</property>
				<property>/b707/generator/gen-control-cover[1]</property>
				<property>/b707/generator/gen-control-cover[2]</property>
				<property>/b707/generator/gen-control-cover[3]</property>
			</condition>
		</error>	
		<exit>
			<condition>
				<property>/b707/generator/gen-control[0]</property>
				<property>/b707/generator/gen-control[1]</property>
				<property>/b707/generator/gen-control[2]</property>
				<property>/b707/generator/gen-control[3]</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			GEN - BREAKER
			Close all circuits  
		</message>
		<view>
				<heading-offset-deg>246.5</heading-offset-deg>
				<pitch-offset-deg>8.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>17.8</field-of-view>
		</view>

		<marker>
				<x-m>-17.8521</x-m>
				<y-m>0.6661</y-m>
				<z-m>1.3331</z-m>
				<scale>1.8430</scale>
		</marker>
		<error>
			<message>
				Close all circuits GEN-BREAKER, now!
			</message>
			<condition>
				<not><property>/b707/generator/gen-breaker[0]</property></not>
				<not><property>/b707/generator/gen-breaker[1]</property></not>
				<not><property>/b707/generator/gen-breaker[2]</property></not>
				<not><property>/b707/generator/gen-breaker[3]</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/generator/gen-breaker[0]</property>
				<property>/b707/generator/gen-breaker[1]</property>
				<property>/b707/generator/gen-breaker[2]</property>
				<property>/b707/generator/gen-breaker[3]</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Sync every CROSSFEED VALVE to his shut (blue lights out) 
			Turn on and off all valves for sec. 
		</message>
		<view>
				<heading-offset-deg>244.9</heading-offset-deg>
				<pitch-offset-deg>-9.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>31.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.8157</x-m>
				<y-m>0.7496</y-m>
				<z-m>0.9017</z-m>
				<scale>1.8595</scale>
		</marker>

		<error>
			<message>
				Open and close the Crossfeed - valves once!
			</message>
			<condition>
				<not><property>/b707/fuel/valves/valve-pos[0]</property></not>
				<not><property>/b707/fuel/valves/valve-pos[1]</property></not>
				<not><property>/b707/fuel/valves/valve-pos[2]</property></not>
				<not><property>/b707/fuel/valves/valve-pos[3]</property></not>
				<not><property>/b707/fuel/valves/valve-pos[4]</property></not>
				<not><property>/b707/fuel/valves/valve-pos[5]</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/fuel/valves/valve-pos[0]</property>
				<property>/b707/fuel/valves/valve-pos[1]</property>
				<property>/b707/fuel/valves/valve-pos[2]</property>
				<property>/b707/fuel/valves/valve-pos[3]</property>
				<property>/b707/fuel/valves/valve-pos[4]</property>
				<property>/b707/fuel/valves/valve-pos[5]</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Switch on the BOOST - PUMPS 
		</message>
		<view>
				<heading-offset-deg>244.9</heading-offset-deg>
				<pitch-offset-deg>-9.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>31.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.8074</x-m>
				<y-m>0.7496</y-m>
				<z-m>1.0231</z-m>
				<scale>3.0496</scale>
		</marker>

		<error>
			<message>
				Set every Boost-pump to on!
			</message>
			<condition>
				<not><property>/b707/fuel/valves/boost-pump[0]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[1]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[2]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[3]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[4]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[5]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[6]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[7]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[8]</property></not>
				<not><property>/b707/fuel/valves/boost-pump[9]</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/fuel/valves/boost-pump[0]</property>
				<property>/b707/fuel/valves/boost-pump[1]</property>
				<property>/b707/fuel/valves/boost-pump[2]</property>
				<property>/b707/fuel/valves/boost-pump[3]</property>
				<property>/b707/fuel/valves/boost-pump[4]</property>
				<property>/b707/fuel/valves/boost-pump[5]</property>
				<property>/b707/fuel/valves/boost-pump[6]</property>
				<property>/b707/fuel/valves/boost-pump[7]</property>
				<property>/b707/fuel/valves/boost-pump[8]</property>
				<property>/b707/fuel/valves/boost-pump[9]</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Set every ENGINE SHUTOFF - VALVE to ON 
		</message>
		<view>
				<heading-offset-deg>244.9</heading-offset-deg>
				<pitch-offset-deg>-9.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>31.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.8174</x-m>
				<y-m>0.7496</y-m>
				<z-m>1.1000</z-m>
				<scale>3.0496</scale>
		</marker>

		<error>
			<message>
				ALL engine SHUTOFF-Valves must be set to on.
			</message>
			<condition>
				<not><property>/b707/fuel/valves/fuel-shutoff[0]</property></not>
				<not><property>/b707/fuel/valves/fuel-shutoff[1]</property></not>
				<not><property>/b707/fuel/valves/fuel-shutoff[2]</property></not>
				<not><property>/b707/fuel/valves/fuel-shutoff[3]</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/fuel/valves/fuel-shutoff[0]</property>
				<property>/b707/fuel/valves/fuel-shutoff[1]</property>
				<property>/b707/fuel/valves/fuel-shutoff[2]</property>
				<property>/b707/fuel/valves/fuel-shutoff[3]</property>
			</condition>
		</exit>
	</step>
		
	<step>
		<message>Open cover Starter 3</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<marker>
		  <x-m> 0.0322</x-m>
		  <y-m> 0.0393</y-m>
		  <z-m> 0.1301</z-m>
			<scale>3.0000</scale>
		</marker>
		<exit>
			<condition>
					<property>/b707/start/startercover[2]</property>
			</condition>
		</exit>
	</step>

	<step>
		<message>Push Starter 3 and then pull cutoff.</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<marker>
				<x-m>-18.3301</x-m>
				<y-m>0.0149</y-m>
				<z-m>1.4176</z-m>
				<scale>1.9107</scale>
		</marker>
		<exit>
			<condition>
				<property>engines/engine[2]/starter</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Pull CUTOFF 3.
		</message>
		<view>
				<heading-offset-deg>300.2</heading-offset-deg>
				<pitch-offset-deg>-38.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>31.1</field-of-view>
		</view>

		<marker>
				<x-m>-18.5140</x-m>
				<y-m>0.0074</y-m>
				<z-m>0.6669</z-m>
				<scale>3.6628</scale>
		</marker>

		<error>
			<message>
				pull lever 3!
			</message>
			<condition>
				<property>controls/engines/engine[2]/cutoff</property>
			</condition>
		</error>
		<exit>
			<condition>
				<not><property>controls/engines/engine[2]/cutoff</property></not>
			</condition>
		</exit>
	</step>

	<step>
		<message>Control N2 and the other instrument for this engine</message>
		<view>
				<heading-offset-deg>319.3</heading-offset-deg>
				<pitch-offset-deg>-28.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>52.9</field-of-view>
		</view>

		<marker>
				<x-m>-18.9037</x-m>
				<y-m>-0.0017</y-m>
				<z-m>0.8449</z-m>
				<scale>1.9107</scale>
		</marker>
		<exit>
			<condition>
				<greater-than>
					<property>engines/engine[2]/n2</property>
					<value>35</value>
				</greater-than>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Starter 3 - green light is out?</message>
		<view>
				<heading-offset-deg>315.9</heading-offset-deg>
				<pitch-offset-deg>-29.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>39.1</field-of-view>
		</view>

		<marker>
				<x-m>-18.3301</x-m>
				<y-m>0.0149</y-m>
				<z-m>1.4176</z-m>
				<scale>1.9107</scale>
		</marker>

		<exit>
			<condition>
				<property>engines/engine[2]/running</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Close cover 3, open cover 4</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<exit>
			<condition>
				<property>engines/engine[2]/running</property>
				<property>/b707/start/startercover[3]</property>
			</condition>
		</exit>
	</step>

	<step>
		<message>Push Starter 4 and then pull cutoff.</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<marker>
				<x-m>-18.3301</x-m>
				<y-m>0.0719</y-m>
				<z-m>1.4176</z-m>
				<scale>1.9107</scale>
		</marker>
		<exit>
			<condition>
				<property>engines/engine[3]/starter</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Pull CUTOFF 4.
		</message>
		<view>
				<heading-offset-deg>300.2</heading-offset-deg>
				<pitch-offset-deg>-38.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>31.1</field-of-view>
		</view>

		<marker>
				<x-m>-18.5140</x-m>
				<y-m>0.0074</y-m>
				<z-m>0.6669</z-m>
				<scale>3.6628</scale>
		</marker>

		<error>
			<message>
				pull lever 4!
			</message>
			<condition>
				<property>controls/engines/engine[3]/cutoff</property>
			</condition>
		</error>
		<exit>
			<condition>
				<not><property>controls/engines/engine[3]/cutoff</property></not>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Control N2 and the other instrument for this engine</message>
		<view>
				<heading-offset-deg>319.3</heading-offset-deg>
				<pitch-offset-deg>-28.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>52.9</field-of-view>
		</view>

		<marker>
				<x-m>-18.9037</x-m>
				<y-m>0.0380</y-m>
				<z-m>0.8449</z-m>
				<scale>1.9107</scale>
		</marker>

		<exit>
			<condition>
				<greater-than>
					<property>engines/engine[3]/n2</property>
					<value>40</value>
				</greater-than>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Starter 4 - wait until green light is out</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<exit>
			<condition>
				<property>engines/engine[3]/running</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Close cover 4, open cover 2</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<exit>
			<condition>
				<property>engines/engine[3]/running</property>
				<property>/b707/start/startercover[1]</property>
			</condition>
		</exit>
	</step>

	<step>
		<message>Push Starter 2 and then pull cutoff.</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<marker>
				<x-m>-18.3301</x-m>
				<y-m>-0.0565</y-m>
				<z-m>1.4102</z-m>
				<scale>1.9107</scale>
		</marker>
		<exit>
			<condition>
				<property>engines/engine[1]/starter</property>
			</condition>
		</exit>
	</step>
		
	<step>
		<message>
			Pull CUTOFF 2.
		</message>
		<view>
				<heading-offset-deg>300.2</heading-offset-deg>
				<pitch-offset-deg>-38.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>31.1</field-of-view>
		</view>

		<marker>
				<x-m>-18.5140</x-m>
				<y-m>0.0074</y-m>
				<z-m>0.6669</z-m>
				<scale>3.6628</scale>
		</marker>

		<error>
			<message>
				pull lever 2!
			</message>
			<condition>
				<property>controls/engines/engine[1]/cutoff</property>
			</condition>
		</error>
		<exit>
			<condition>
				<not><property>controls/engines/engine[1]/cutoff</property></not>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Control N2 and the other instrument for this engine</message>
		<view>
				<heading-offset-deg>319.3</heading-offset-deg>
				<pitch-offset-deg>-28.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>52.9</field-of-view>
		</view>

		<marker>
				<x-m>-18.9037</x-m>
				<y-m>-0.0430</y-m>
				<z-m>0.8449</z-m>
				<scale>1.9107</scale>
		</marker>

		<exit>
			<condition>
				<greater-than>
					<property>engines/engine[1]/n2</property>
					<value>40</value>
				</greater-than>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Starter 2 - wait until green light is out</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<exit>
			<condition>
				<property>engines/engine[1]/running</property>
			</condition>
		</exit>
	</step>	
	
	<step>
		<message>Close cover 2, open cover 1</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<exit>
			<condition>
				<property>engines/engine[1]/running</property>
				<property>/b707/start/startercover[0]</property>
			</condition>
		</exit>
	</step>

	<step>
		<message>Push Starter 1 and then pull cutoff.</message>
		<view>
				<heading-offset-deg>292.9</heading-offset-deg>
				<pitch-offset-deg>27.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>47.4</field-of-view>
		</view>
		<marker>
				<x-m>-18.3301</x-m>
				<y-m>-0.1193</y-m>
				<z-m>1.4102</z-m>
				<scale>1.9107</scale>
		</marker>
		<exit>
			<condition>
				<property>engines/engine[0]/starter</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Pull CUTOFF 1.
		</message>
		<view>
				<heading-offset-deg>300.2</heading-offset-deg>
				<pitch-offset-deg>-38.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>31.1</field-of-view>
		</view>

		<marker>
				<x-m>-18.5140</x-m>
				<y-m>0.0074</y-m>
				<z-m>0.6669</z-m>
				<scale>3.6628</scale>
		</marker>

		<error>
			<message>
				pull lever 1!
			</message>
			<condition>
				<property>controls/engines/engine[0]/cutoff</property>
			</condition>
		</error>
		<exit>
			<condition>
				<not><property>controls/engines/engine[0]/cutoff</property></not>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Control N2 and the other instrument for this engine</message>
		<view>
				<heading-offset-deg>319.3</heading-offset-deg>
				<pitch-offset-deg>-28.3</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.5</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>52.9</field-of-view>
		</view>

		<marker>
				<x-m>-18.9037</x-m>
				<y-m>-0.0843</y-m>
				<z-m>0.8449</z-m>
				<scale>1.9107</scale>
		</marker>

		<exit>
			<condition>
				<greater-than>
					<property>engines/engine[1]/n2</property>
					<value>35</value>
				</greater-than>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>Starter 1 - wait until green light is out</message>
		<view>
			<heading-offset-deg>-75</heading-offset-deg>
			<pitch-offset-deg>30.0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.46</x-offset-m>
			<y-offset-m>1.19</y-offset-m>
			<z-offset-m>-18.2</z-offset-m>
			<field-of-view>44.3</field-of-view>
		</view>
		<exit>
			<condition>
				<property>engines/engine[0]/running</property>
			</condition>
		</exit>
	</step>	

	<step>
		<message>Close cover 1</message>
		<view>
			<heading-offset-deg>-75</heading-offset-deg>
			<pitch-offset-deg>30.0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.46</x-offset-m>
			<y-offset-m>1.19</y-offset-m>
			<z-offset-m>-18.2</z-offset-m>
			<field-of-view>44.3</field-of-view>
		</view>
		<exit>
			<condition>
				<not><property>/b707/start/startercover[0]</property></not>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>control N2 in green range.</message>
		<view>
			<heading-offset-deg>-40.0</heading-offset-deg>
			<pitch-offset-deg>-20.0</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.46</x-offset-m>
			<y-offset-m>1.19</y-offset-m>
			<z-offset-m>-18.2</z-offset-m>
			<field-of-view>44.3</field-of-view>
		</view>
		<exit>
			<condition>
				<greater-than>
					<property>engines/engine[0]/n2</property>
					<value>50</value>
				</greater-than>
				<greater-than>
					<property>engines/engine[1]/n2</property>
					<value>50</value>
				</greater-than>
				<greater-than>
					<property>engines/engine[2]/n2</property>
					<value>50</value>
				</greater-than>
				<greater-than>
					<property>engines/engine[3]/n2</property>
					<value>50</value>
				</greater-than>
			</condition>
		</exit>
	</step>
		
	<step>
		<message>
			SELECTOR AC PARALLELING select GEN I
			We will synchronize the generators now.
		</message>
		<view>
				<heading-offset-deg>244.2</heading-offset-deg>
				<pitch-offset-deg>4.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>20.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.6066</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2455</z-m>
				<scale>1.6612</scale>
		</marker>

		<error>
			<message>Select GEN I</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ac/ac-para-select</property>
						<value>1</value>
					</less-than>
					<greater-than>
						<property>/b707/ac/ac-para-select</property>
						<value>1</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ac/ac-para-select</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Heed this instrument during synchronisation
		</message>
		<view>
				<heading-offset-deg>244.2</heading-offset-deg>
				<pitch-offset-deg>4.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>20.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.6182</x-m>
				<y-m>0.6513</y-m>
				<z-m>1.3107</z-m>
				<scale>2.5372</scale>
		</marker>
	</step>

	<step>
		<message>
			Turn FREQ CONTROL knob until white control lights are out.
		</message>
		<view>
				<heading-offset-deg>247.7</heading-offset-deg>
				<pitch-offset-deg>4.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>21.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.8314</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2174</z-m>
				<scale>1.7934</scale>
		</marker>
		<error>
			<message>synchronize generator 1 now</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/generator/gen-freq[0]</property>
						<value>400</value>
					</less-than>
					<greater-than>
						<property>/b707/generator/gen-freq[0]</property>
						<value>400</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/generator/gen-freq[0]</property>
					<value>400</value>
				</equals>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Select GEN 2 at SELECTOR AC PARALLELING
		</message>
		<view>
				<heading-offset-deg>244.2</heading-offset-deg>
				<pitch-offset-deg>4.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>20.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.6066</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2455</z-m>
				<scale>1.6612</scale>
		</marker>

		<error>
			<message>select GEN 2</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ac/ac-para-select</property>
						<value>2</value>
					</less-than>
					<greater-than>
						<property>/b707/ac/ac-para-select</property>
						<value>2</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ac/ac-para-select</property>
					<value>2</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Turn FREQ CONTROL knob until white control lights are out
		</message>
		<view>
				<heading-offset-deg>247.7</heading-offset-deg>
				<pitch-offset-deg>4.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>21.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.7785</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2174</z-m>
				<scale>1.7934</scale>
		</marker>
		<error>
			<message>synchronize generator 2 now</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/generator/gen-freq[1]</property>
						<value>400</value>
					</less-than>
					<greater-than>
						<property>/b707/generator/gen-freq[1]</property>
						<value>400</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/generator/gen-freq[1]</property>
					<value>400</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Select GEN 3 at SELECTOR AC PARALLELING
		</message>
		<view>
				<heading-offset-deg>244.2</heading-offset-deg>
				<pitch-offset-deg>4.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>20.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.5719</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2695</z-m>
				<scale>1.6612</scale>
		</marker>

		<error>
			<message>select GEN 3</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ac/ac-para-select</property>
						<value>4</value>
					</less-than>
					<greater-than>
						<property>/b707/ac/ac-para-select</property>
						<value>4</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ac/ac-para-select</property>
					<value>4</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Turn FREQ CONTROL knob until white control lights are out
		</message>
		<view>
				<heading-offset-deg>247.7</heading-offset-deg>
				<pitch-offset-deg>4.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>21.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.7248</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2149</z-m>
				<scale>1.7934</scale>
		</marker>
		<error>
			<message>synchronize generator 3 now</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/generator/gen-freq[2]</property>
						<value>400</value>
					</less-than>
					<greater-than>
						<property>/b707/generator/gen-freq[2]</property>
						<value>400</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/generator/gen-freq[2]</property>
					<value>400</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Set SELECTOR AC PARALLELING to GEN 4
		</message>
		<view>
				<heading-offset-deg>244.2</heading-offset-deg>
				<pitch-offset-deg>4.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>20.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.5719</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2695</z-m>
				<scale>1.6612</scale>
		</marker>

		<error>
			<message>Select gen 4</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ac/ac-para-select</property>
						<value>5</value>
					</less-than>
					<greater-than>
						<property>/b707/ac/ac-para-select</property>
						<value>5</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ac/ac-para-select</property>
					<value>5</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Turn FREQ CONTROL knob until white control lights are out
		</message>
		<view>
				<heading-offset-deg>247.7</heading-offset-deg>
				<pitch-offset-deg>4.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>21.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.6719</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2149</z-m>
				<scale>1.7934</scale>
		</marker>
		<error>
			<message>synchronize generator 4 now</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/generator/gen-freq[3]</property>
						<value>400</value>
					</less-than>
					<greater-than>
						<property>/b707/generator/gen-freq[3]</property>
						<value>400</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/generator/gen-freq[3]</property>
					<value>400</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Select GEN 1 on SELECTOR AC PARALLELING for controlling
		</message>
		<view>
				<heading-offset-deg>244.2</heading-offset-deg>
				<pitch-offset-deg>4.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>20.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.6066</x-m>
				<y-m>0.7000</y-m>
				<z-m>1.2455</z-m>
				<scale>1.6612</scale>
		</marker>

		<error>
			<message>turn to GEN 1</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ac/ac-para-select</property>
						<value>1</value>
					</less-than>
					<greater-than>
						<property>/b707/ac/ac-para-select</property>
						<value>1</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ac/ac-para-select</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Close all BUS-TIE-BREAKER, now
		</message>
		<view>
				<heading-offset-deg>244.9</heading-offset-deg>
				<pitch-offset-deg>9.7</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>16.7</field-of-view>
		</view>

		<marker>
				<x-m>-17.8653</x-m>
				<y-m>0.5992</y-m>
				<z-m>1.3669</z-m>
				<scale>1.6628</scale>
		</marker>
		<error>
			<message>
				close all busses!
			</message>
			<condition>
				<not><property>/b707/generator/gen-bus-tie[0]</property></not>
				<not><property>/b707/generator/gen-bus-tie[1]</property></not>
				<not><property>/b707/generator/gen-bus-tie[2]</property></not>
				<not><property>/b707/generator/gen-bus-tie[3]</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/generator/gen-bus-tie[0]</property>
				<property>/b707/generator/gen-bus-tie[1]</property>
				<property>/b707/generator/gen-bus-tie[2]</property>
				<property>/b707/generator/gen-bus-tie[3]</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Our essential power source is generator 1 now.
			Turn knob to GEN I
		</message>
		<view>
				<heading-offset-deg>238.1</heading-offset-deg>
				<pitch-offset-deg>7.5</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>14.5</field-of-view>
		</view>

		<marker>
				<x-m>-17.5620</x-m>
				<y-m>0.6000</y-m>
				<z-m>1.3686</z-m>
				<scale>1.3967</scale>
		</marker>
		<error>
			<message>Turn to generator 1</message>
			<condition>
				<or>
					<less-than>
						<property>/b707/ess-power-switch</property>
						<value>1</value>
					</less-than>
					<greater-than>
						<property>/b707/ess-power-switch</property>
						<value>1</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<equals>
					<property>/b707/ess-power-switch</property>
					<value>1</value>
				</equals>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Cutoff connection to the power unit
		</message>
		<view>
				<heading-offset-deg>237.8</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.3</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>15.9</field-of-view>
		</view>

		<marker>
				<x-m>-17.5785</x-m>
				<y-m>0.6000</y-m>
				<z-m>1.4091</z-m>
				<scale>1.4959</scale>
		</marker>
		<error>
			<message>
				switch to OFF.
			</message>
			<condition>
				<property>/b707/ground-connect</property>
			</condition>
		</error>
		<exit>
			<condition>
				<not><property>/b707/ground-connect</property></not>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Unplug external power unit now
			Select in the main menu: Boeing 707/ External Power Unit
		</message>
		<view>
				<heading-offset-deg>240.8</heading-offset-deg>
				<pitch-offset-deg>4.0</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>49.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.5636</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.3967</z-m>
				<scale>1.6612</scale>
		</marker>

		<exit>
			<condition>
				<not><property>/b707/external-power-connected</property></not>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			External power unit is switch off
		</message>
		<view>
			<view-number>1</view-number>
			<heading-offset-deg>182.1</heading-offset-deg>
			<pitch-offset-deg>-4.6</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>0.3</x-offset-m>
			<y-offset-m>1.8</y-offset-m>
			<z-offset-m>-32.0</z-offset-m>
			<field-of-view>70</field-of-view>
		</view>
		<exit>
			<condition>
				<not><property>/b707/external-power-connected</property></not>
			</condition>
		</exit>
	</step>
	
	
	<step>
		<message>
			40 Hertz Converter - Controls 115Volt 60 cycle power to the stateroom and the number two galley areas.
		</message>
		<view>
			<heading-offset-deg>239.9</heading-offset-deg>
			<pitch-offset-deg>-4.9</pitch-offset-deg>
			<roll-offset-deg>0.0</roll-offset-deg>
			<x-offset-m>-0.4</x-offset-m>
			<y-offset-m>1.2</y-offset-m>
			<z-offset-m>-18.2</z-offset-m>
			<field-of-view>28.6</field-of-view>
		</view>

		<marker>
			<x-m>-17.5876</x-m>
			<y-m>0.5711</y-m>
			<z-m>1.0636</z-m>
			<scale>1.6612</scale>
		</marker>
		<error>
			<message>
				Switch to ON.
			</message>
			<condition>
				<not><property>/b707/generator/hertz-converter</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/generator/hertz-converter</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Set the Equipment Cooling pumps to ON.
		</message>
		<view>
				<heading-offset-deg>239.9</heading-offset-deg>
				<pitch-offset-deg>-4.9</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>28.6</field-of-view>
		</view>

		<marker>
				<x-m>-17.5876</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.1157</z-m>
				<scale>1.6612</scale>
		</marker>

		<error>
			<message>
				Both switch to ON.
			</message>
			<condition>
				<not><property>/b707/equipment/ovbd-dump</property></not>
				<not><property>/b707/equipment/blower</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/equipment/ovbd-dump</property>
				<property>/b707/equipment/blower</property>
			</condition>
		</exit>
	</step>
	
	<step>
		<message>
			Open the cover for the RAM Air and switch it on.
		</message>
		<view>
				<heading-offset-deg>229.9</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>30.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.3264</x-m>
				<y-m>0.5356</y-m>
				<z-m>1.4959</z-m>
				<scale>2.3224</scale>
		</marker>

		<error>
			<message>
				Set switch to OPEN.
			</message>
			<condition>
				<not><property>/b707/air-conditioning/ram-air-switch</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/air-conditioning/ram-air-switch</property>
			</condition>
		</exit>
	</step>	

	<step>
		<message>
			Start Air Compressor on engine 2.
		</message>
		<view>
				<heading-offset-deg>229.9</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>30.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.5041</x-m>
				<y-m>0.5356</y-m>
				<z-m>1.4579</z-m>
				<scale>2.3224</scale>
		</marker>
		<error>
			<message>
				Switch to START. If RPM is over 115% restart the compressor.
			</message>
			<condition>
				<not><property>/b707/air-conditioning/compressor-start[0]</property></not>
				<greater-than>
					<property>/b707/air-conditioning/compressor-rpm[0]</property>
					<value>115</value>
				</greater-than>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/air-conditioning/compressor-start[0]</property>
				<less-than>
					<property>/b707/air-conditioning/compressor-rpm[0]</property>
					<value>115</value>
				</less-than>
				<greater-than>
					<property>/b707/air-conditioning/compressor-rpm[0]</property>
					<value>90</value>
				</greater-than>	
			</condition>
		</exit>
	</step>	

	<step>
		<message>
			Start Air Compressor on engine 3.
		</message>
		<view>
				<heading-offset-deg>229.9</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>30.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.4537</x-m>
				<y-m>0.5356</y-m>
				<z-m>1.4579</z-m>
				<scale>2.3224</scale>
		</marker>
		<error>
			<message>
				Switch to START. If RPM is over 115% restart the compressor.
				Also watch the amber lights of compressor 1. Restart if necessary the first one.
			</message>
			<condition>
				<not><property>/b707/air-conditioning/compressor-start[1]</property></not>
				<or>			
					<greater-than>
						<property>/b707/air-conditioning/compressor-rpm[1]</property>
						<value>115</value>
					</greater-than>				
					<greater-than>
						<property>/b707/air-conditioning/compressor-rpm[0]</property>
						<value>115</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/air-conditioning/compressor-start[1]</property>
				<less-than>
					<property>/b707/air-conditioning/compressor-rpm[1]</property>
					<value>115</value>
				</less-than>
				<greater-than>
					<property>/b707/air-conditioning/compressor-rpm[1]</property>
					<value>90</value>
				</greater-than>	
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Start Air Compressor on engine 4.
		</message>
		<view>
				<heading-offset-deg>229.9</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>30.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.4041</x-m>
				<y-m>0.5356</y-m>
				<z-m>1.4579</z-m>
				<scale>2.3224</scale>
		</marker>
		<error>
			<message>
				Switch to START. If RPM is over 115% restart the compressor.
				Also watch the amber lights of compressors 1 and 2. Restart if necessary those.
			</message>
			<condition>
				<not><property>/b707/air-conditioning/compressor-start[2]</property></not>
				<or>
					<greater-than>
						<property>/b707/air-conditioning/compressor-rpm[2]</property>
						<value>115</value>
					</greater-than>				
					<greater-than>
						<property>/b707/air-conditioning/compressor-rpm[1]</property>
						<value>115</value>
					</greater-than>				
					<greater-than>
						<property>/b707/air-conditioning/compressor-rpm[0]</property>
						<value>115</value>
					</greater-than>
				</or>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/air-conditioning/compressor-start[2]</property>
				<less-than>
					<property>/b707/air-conditioning/compressor-rpm[2]</property>
					<value>115</value>
				</less-than>
				<greater-than>
					<property>/b707/air-conditioning/compressor-rpm[2]</property>
					<value>90</value>
				</greater-than>	
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Switch on the WING VALVES.
		</message>
		<view>
				<heading-offset-deg>229.9</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>30.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.4801</x-m>
				<y-m>0.5356</y-m>
				<z-m>1.4166</z-m>
				<scale>2.3224</scale>
		</marker>
		<error>
			<message>
				Open the cross-body-duct, L and R to OPEN.
			</message>
			<condition>
				<not><property>/b707/air-conditioning/wing-valve[0]</property></not>
				<not><property>/b707/air-conditioning/wing-valve[1]</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/air-conditioning/wing-valve[0]</property>
				<property>/b707/air-conditioning/wing-valve[1]</property>
			</condition>
		</exit>
	</step>

	<step>
		<message>
			Open the air conditioning unit switches. First open the cover.
		</message>
		<view>
				<heading-offset-deg>229.9</heading-offset-deg>
				<pitch-offset-deg>8.2</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>30.1</field-of-view>
		</view>

		<marker>
				<x-m>-17.4933</x-m>
				<y-m>0.5356</y-m>
				<z-m>1.3620</z-m>
				<scale>3.2811</scale>
		</marker>
		<error>
			<message>
				Open both air conditioning units. Set to ON.
			</message>
			<condition>
				<not><property>/b707/air-conditioning/air-cond-unit-left-start</property></not>
				<not><property>/b707/air-conditioning/air-cond-unit-right-start</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/air-conditioning/air-cond-unit-left-start</property>
				<property>/b707/air-conditioning/air-cond-unit-right-start</property>
			</condition>
		</exit>
	</step>	

	<step>
		<message>
			Open the cover of the Safety-Air-valve.
			Switch the knob to the bottom. 
		</message>
		<view>
				<heading-offset-deg>227.6</heading-offset-deg>
				<pitch-offset-deg>3.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>23.5</field-of-view>
		</view>

		<marker>
				<x-m>-17.1619</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.3967</z-m>
				<scale>2.3224</scale>
		</marker>

		<error>
			<message>
				Switch down the knob, the amber light extinguished.
			</message>
			<condition>
				<not><property>/b707/pressurization/safety-valve</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/pressurization/safety-valve</property>
			</condition>
		</exit>
	</step>		
	
	<step>
		<message>
			Now switch on the Pressurization Auto Mode. 
		</message>
		<view>
				<heading-offset-deg>227.6</heading-offset-deg>
				<pitch-offset-deg>3.8</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>23.5</field-of-view>
		</view>

		<marker>
				<x-m>-17.4264</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.2380</z-m>
				<scale>1.8100</scale>
		</marker>
		<error>
			<message>
				Set switch to ON.
			</message>
			<condition>
				<not><property>/b707/pressurization/manual-mode-switch</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/pressurization/manual-mode-switch</property>
			</condition>
		</exit>
	</step>	

	<step>
		<message>
			Chose take off position. 
		</message>
		<view>
				<heading-offset-deg>235.3</heading-offset-deg>
				<pitch-offset-deg>1.4</pitch-offset-deg>
				<roll-offset-deg>0.0</roll-offset-deg>
				<x-offset-m>-0.4</x-offset-m>
				<y-offset-m>1.2</y-offset-m>
				<z-offset-m>-18.2</z-offset-m>
				<field-of-view>14.3</field-of-view>
		</view>

		<marker>
				<x-m>-17.5785</x-m>
				<y-m>0.5711</y-m>
				<z-m>1.2380</z-m>
				<scale>1.1488</scale>
		</marker>
		<error>
			<message>
				Set switch to on.
			</message>
			<condition>
				<not><property>/b707/pressurization/mode-switch</property></not>
			</condition>
		</error>
		<exit>
			<condition>
				<property>/b707/pressurization/mode-switch</property>
			</condition>
		</exit>
	</step>	
			
	<end>
		<message>All engines started. Generators closed. Have a nice trip!</message>
		<view>
			<heading-offset-deg>0</heading-offset-deg>
			<pitch-offset-deg>-16</pitch-offset-deg>
			<field-of-view>72</field-of-view>
		</view>
	</end>

</PropertyList>
