<?xml version="1.0" encoding="UTF-8"?>
<!--###################################################################################
        Lake of Constance Hangar :: M.Kraus
        Boeing 707 for Flightgear Septemper 2013
        This file is licenced under the terms of the GNU General Public Licence V2 or later
        ###################################################################################
-->
<PropertyList>
    <name>Engines: Start-up [portugues]</name>
    <description>Motores de arranque, com unidade de alimentacao externa.</description>
 
    <init>
        <set>
            <property>/sim/current-view/view-number</property>
            <value>0</value>
        </set>
        <set>
            <property>/controls/gear/brake-parking</property>
            <value>1</value>
        </set>
        <set>
            <property>/controls/flight/flaps</property>
            <value>0.0</value>
        </set>
        <set>
            <property>/b707/generator/gen-bus-tie[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-breaker[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-control[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-drive[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-bus-tie[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-breaker[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-control[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-drive[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-bus-tie[2]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-breaker[2]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-control[2]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-drive[2]</property>
            <value>0</value>
        </set>
        <set>
            <property>/controls/electric/engine[2]/generator</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-bus-tie[3]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-breaker[3]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-control[3]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/generator/gen-drive[3]</property>
            <value>0</value>
        </set>
        <set>
            <property>/controls/engines/engine[0]/cutoff</property>
            <value>1</value>
        </set>
        <set>
            <property>/controls/engines/engine[1]/cutoff</property>
            <value>1</value>
        </set>
        <set>
            <property>/controls/engines/engine[2]/cutoff</property>
            <value>1</value>
        </set>
        <set>
            <property>/controls/engines/engine[3]/cutoff</property>
            <value>1</value>
        </set>
        <set>
            <property>/b707/fuel/valves/valve-pos[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/valve-pos[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/valve-pos[2]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/valve-pos[3]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/valve-pos[4]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/valve-pos[5]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[3]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[4]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[5]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[6]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[7]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[8]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/boost-pump[9]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/fuel-shutoff[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/fuel-shutoff[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/fuel-shutoff[2]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/fuel/valves/fuel-shutoff[3]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/load-volt-selector</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/external-power-connected</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/battery-switch</property>
            <value>0</value>
        </set>        
        <set>
            <property>/b707/hydraulic/rudder</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/system</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/brake-valve</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/ac-aux-pump[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/ac-aux-pump[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/hyd-fluid-shutoff-cover[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/hyd-fluid-shutoff-cover[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/hyd-fluid-shutoff[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/hyd-fluid-shutoff[1]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/hyd-fluid-pump[0]</property>
            <value>0</value>
        </set>
        <set>
            <property>/b707/hydraulic/hyd-fluid-pump[1]</property>
            <value>0</value>
        </set>
    </init>
    <step>
        <message>
           Conecte a unidade de alimentacao externa.
           No menu principal B707/ unidade de alimentacao externa
        </message>
        <view>
                <heading-offset-deg>240.8</heading-offset-deg>
                <pitch-offset-deg>4.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>49.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.5636</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.3967</z-m>
                <scale>1.6612</scale>
        </marker>
        <exit>
            <condition>
                <property>/b707/external-power-connected</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
            Unidade de alimentacao externa foi conectada.
        </message>
        <view>
            <view-number>1</view-number>
                <heading-offset-deg>195.9</heading-offset-deg>
                <pitch-offset-deg>-3.7</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>25.0</x-offset-m>
                <y-offset-m>2.0</y-offset-m>
                <z-offset-m>-45.0</z-offset-m>
                <field-of-view>21.6</field-of-view>
        </view>
        <exit>
            <condition>
                <property>/b707/external-power-connected</property>
            </condition>
        </exit>
    </step> 
    <step>
        <message>
          Ligar a bateria.
        </message>
        <view>
                <heading-offset-deg>235.4</heading-offset-deg>
                <pitch-offset-deg>7.9</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>51.5</field-of-view>
        </view>
        <marker>
                <x-m>-17.5901</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.4587</z-m>
                <scale>2.3719</scale>
        </marker>
        <error>
            <message>
           Abra a tampa e ligue a bateria.
           </message>
            <condition>
                <not><property>/b707/battery-switch</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/battery-switch</property>
            </condition>
        </exit>
    </step> 
    <step>
        <message>
            Coloque o SELETOR DE CARGAS e VOLTS na posicao de BUS-TIE. Controlador de sincronismo automatico
        </message>
        <view>
                <heading-offset-deg>234.0</heading-offset-deg>
                <pitch-offset-deg>14.4</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>14.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.5554</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.4628</z-m>
                <scale>3.0000</scale>
        </marker>
        <error>
            <message>
             Use somente BUS TIE no momento.
             </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/load-volt-selector</property>
                        <value>1</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/load-volt-selector</property>
                        <value>1</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/load-volt-selector</property>
                    <value>1</value>
                </equals>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            POTENCIA BASICA iniciar POTENCIA EXTERNA.
        </message>
        <view>
                <heading-offset-deg>238.1</heading-offset-deg>
                <pitch-offset-deg>7.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>14.5</field-of-view>
        </view>
        <marker>
                <x-m>-17.5620</x-m>
                <y-m>0.6000</y-m>
                <z-m>1.3686</z-m>
                <scale>1.3967</scale>
        </marker>
        <error>
            <message>
            Iniciar EXT PWR(potencia externa).
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ess-power-switch</property>
                        <value>5</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ess-power-switch</property>
                        <value>5</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ess-power-switch</property>
                    <value>5</value>
                </equals>
            </condition>
        </exit>
    </step>   
    <step>
        <message>	
         SELETOR AC PARALELO definido como a fonte de alimentacao externa.
         A fonte de AC sera sincronizada para 400Hz.
        </message>
        <view>
                <heading-offset-deg>241.4</heading-offset-deg>
                <pitch-offset-deg>3.4</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>15.9</field-of-view>
        </view>
        <marker>
                <x-m>-17.6165</x-m>
                <y-m>0.6000</y-m>
                <z-m>1.2488</z-m>
                <scale>1.3967</scale>
        </marker>
        <error>
            <message>
            selecione External Power(alimentacao externa).
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>6</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>6</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ac/ac-para-select</property>
                    <value>6</value>
                </equals>
            </condition>
        </exit>
    </step>
    <step>
        <message>
            BOMBAS auxiliares ON.
            Pressao hidraulica para leme equipamento e sistema de apoio.
        </message>
        <view>
                <heading-offset-deg>230.5</heading-offset-deg>
                <pitch-offset-deg>-17.6</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>17.7</field-of-view>
        </view>
        <marker>
                <x-m>-17.4422</x-m>
                <y-m>0.7289</y-m>
                <z-m>0.7942</z-m>
                <scale>1.4959</scale>
        </marker>
        <error>
            <message>
            Ativar ambos para ON e esperar ate 3000 PSI RUD HYD PRESS.
            </message>
            <condition>
                <or>
                    <not><property>/b707/hydraulic/ac-aux-pump[0]</property></not>
                    <not><property>/b707/hydraulic/ac-aux-pump[1]</property></not>
                    <less-than>
                        <property>/b707/hydraulic/rudder</property>
                        <value>2900</value>
                    </less-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
             <and>
                <property>/b707/hydraulic/ac-aux-pump[0]</property>
                <property>/b707/hydraulic/ac-aux-pump[1]</property>
                <greater-than>
                    <property>/b707/hydraulic/rudder</property>
                    <value>2900</value>
                </greater-than>
             </and>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            VALVULA de interligacao ON.
            Sistema de suporte de bombas auxiliares de AC.
        </message>
        <view>
                <heading-offset-deg>230.5</heading-offset-deg>
                <pitch-offset-deg>-17.6</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>17.7</field-of-view>
        </view>
        <marker>
                <x-m>-17.4066</x-m>
                <y-m>0.7289</y-m>
                <z-m>0.7942</z-m>
                <scale>1.4959</scale>
        </marker>   
        <error>
            <message>      	
            Alternar para baixo este botao
            </message>
            <condition>
                <not>
                    <equals>
                        <property>b707/hydraulic/brake-valve</property>
                        <value>2</value>
                    </equals>
                </not>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>b707/hydraulic/brake-valve</property>
                    <value>2</value>
                </equals>
            </condition>
        </exit>
    </step>            
    <step>
        <message>
            HYD FLUID Dutos on.(Dutos de Fluidos Hidraulicos ON).
        </message>
        <view>
                <heading-offset-deg>230.5</heading-offset-deg>
                <pitch-offset-deg>-17.6</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>17.7</field-of-view>
        </view> 
        <marker>
                <x-m>-17.3207</x-m>
                <y-m>0.7289</y-m>
                <z-m>0.7942</z-m>
                <scale>2.7686</scale>
        </marker>
        <error>
            <message>
            Abra as tampas e ligue os botoes.
            </message>
            <condition>
                <or>
                    <not><property>/b707/hydraulic/hyd-fluid-shutoff[0]</property></not>
                    <not><property>/b707/hydraulic/hyd-fluid-shutoff[1]</property></not>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <and>
                    <property>/b707/hydraulic/hyd-fluid-shutoff[0]</property>
                    <property>/b707/hydraulic/hyd-fluid-shutoff[1]</property>
                </and>
            </condition>
        </exit>
    </step>       
    <step>
        <message>
            BOMBAS de motor ON.
            Suporte hidraulico para todos os sistemas residuais.
        </message>
        <view>
                <heading-offset-deg>230.5</heading-offset-deg>
                <pitch-offset-deg>-17.6</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>17.7</field-of-view>
        </view>
        <marker>
                <x-m>-17.3744</x-m>
                <y-m>0.7289</y-m>
                <z-m>0.7918</z-m>
                <scale>1.5124</scale>
        </marker>
        <error>
            <message>
            Ativar ambos para ON e aguarde ate 2200 PSI HYD SYS PRESS.
            </message>
            <condition>
                <or>
                    <not><property>/b707/hydraulic/hyd-fluid-pump[0]</property></not>
                    <not><property>/b707/hydraulic/hyd-fluid-pump[1]</property></not>                    
                    <less-than>
                        <property>/b707/hydraulic/system</property>
                        <value>2000</value>
                    </less-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <and>
                    <property>/b707/hydraulic/hyd-fluid-pump[0]</property>
                    <property>/b707/hydraulic/hyd-fluid-pump[1]</property>
                    <greater-than>
                        <property>/b707/hydraulic/system</property>
                        <value>2000</value>
                    </greater-than>
                </and>
            </condition>
        </exit>
    </step>       
    <step>
        <message>
            Conectar a unidade de alimentacao externa para o SYNC BUS.(Bus de sincronizacao)
        </message>
        <view>
                <heading-offset-deg>237.8</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>15.9</field-of-view>
        </view>
        <marker>
                <x-m>-17.5785</x-m>
                <y-m>0.6000</y-m>
                <z-m>1.4091</z-m>
                <scale>1.4959</scale>
        </marker>
        <error>
            <message>
                Ativar(ON).
            </message>
            <condition>
                <not><property>/b707/ground-connect</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/ground-connect</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
            Conecte o GEN - DRIVES.
            Abra a tampa vermelha e ligue as unidades. 
            Em seguida feche a tampa.
        </message>
        <view>
                <heading-offset-deg>241.8</heading-offset-deg>
                <pitch-offset-deg>14.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>22.8</field-of-view>
        </view> 
        <marker>
                <x-m>-17.8587</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.4603</z-m>
                <scale>1.6612</scale>
        </marker>
        <error>
            <message>
                Conecte todos os GEN - DRIVES e feche todas as tampas.
                Reconectar em voo e impossivel.
            </message>
            <condition>
                <not><property>/b707/generator/gen-drive[0]</property></not>
                <not><property>/b707/generator/gen-drive[1]</property></not>
                <not><property>/b707/generator/gen-drive[2]</property></not>
                <not><property>/b707/generator/gen-drive[3]</property></not>
                <property>/b707/generator/gen-drive-cover[0]</property>
                <property>/b707/generator/gen-drive-cover[1]</property>
                <property>/b707/generator/gen-drive-cover[2]</property>
                <property>/b707/generator/gen-drive-cover[3]</property>
            </condition>
        </error>        
        <exit>
            <condition>
                <property>/b707/generator/gen-drive[0]</property>
                <property>/b707/generator/gen-drive[1]</property>
                <property>/b707/generator/gen-drive[2]</property>
                <property>/b707/generator/gen-drive[3]</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
            BUS-TIE-BREAKER(BUS de Regulador Automatico de sincronizacao)
            Abra todas as tampas e definir BUS-TIE-BREAKER para sincronizacao bus.
            Em seguida feche a tampa.
        </message>
        <view>
                <heading-offset-deg>244.9</heading-offset-deg>
                <pitch-offset-deg>9.7</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>16.7</field-of-view>
        </view>
        <marker>
                <x-m>-17.8653</x-m>
                <y-m>0.5992</y-m>
                <z-m>1.3669</z-m>
                <scale>1.6628</scale>
        </marker>
        <error>
            <message>   	
            Ligue todos os buses e feche as tampas!
            </message>
            <condition>
                <not><property>/b707/generator/gen-bus-tie[0]</property></not>
                <not><property>/b707/generator/gen-bus-tie[1]</property></not>
                <not><property>/b707/generator/gen-bus-tie[2]</property></not>
                <not><property>/b707/generator/gen-bus-tie[3]</property></not>
                <property>/b707/generator/gen-bus-tie-cover[0]</property>
                <property>/b707/generator/gen-bus-tie-cover[1]</property>
                <property>/b707/generator/gen-bus-tie-cover[2]</property>
                <property>/b707/generator/gen-bus-tie-cover[3]</property>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/generator/gen-bus-tie[0]</property>
                <property>/b707/generator/gen-bus-tie[1]</property>
                <property>/b707/generator/gen-bus-tie[2]</property>
                <property>/b707/generator/gen-bus-tie[3]</property>
            </condition>
        </exit>
    </step>      
    <step>
        <message>
            GEN - CONTROL(controle do gerador)
            Abra todas as tampas e ligar os controladores do gerador.
            Feche em seguida.
        </message>
        <view>
                <heading-offset-deg>246.5</heading-offset-deg>
                <pitch-offset-deg>8.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>17.8</field-of-view>
        </view>
        <marker>
                <x-m>-17.8620</x-m>
                <y-m>0.6661</y-m>
                <z-m>1.2860</z-m>
                <scale>1.8430</scale>
        </marker>
        <error>
            <message>
                Ligue todos os controladores e feche as tampas!
            </message>
            <condition>
                <not><property>/b707/generator/gen-control[0]</property></not>
                <not><property>/b707/generator/gen-control[1]</property></not>
                <not><property>/b707/generator/gen-control[2]</property></not>
                <not><property>/b707/generator/gen-control[3]</property></not>
                <property>/b707/generator/gen-control-cover[0]</property>
                <property>/b707/generator/gen-control-cover[1]</property>
                <property>/b707/generator/gen-control-cover[2]</property>
                <property>/b707/generator/gen-control-cover[3]</property>
            </condition>
        </error>    
        <exit>
            <condition>
                <property>/b707/generator/gen-control[0]</property>
                <property>/b707/generator/gen-control[1]</property>
                <property>/b707/generator/gen-control[2]</property>
                <property>/b707/generator/gen-control[3]</property>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            GEN - BREAKER(REGULADOR AUTOMATICO DO GERADOR)
            Feche todos os circuitos 
        </message>
        <view>
                <heading-offset-deg>246.5</heading-offset-deg>
                <pitch-offset-deg>8.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>17.8</field-of-view>
        </view>
        <marker>
                <x-m>-17.8521</x-m>
                <y-m>0.6661</y-m>
                <z-m>1.3331</z-m>
                <scale>1.8430</scale>
        </marker>
        <error>
            <message>
                Feche todos os circuitos GEN-BREAKER, agora!
            </message>
            <condition>
                <not><property>/b707/generator/gen-breaker[0]</property></not>
                <not><property>/b707/generator/gen-breaker[1]</property></not>
                <not><property>/b707/generator/gen-breaker[2]</property></not>
                <not><property>/b707/generator/gen-breaker[3]</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/generator/gen-breaker[0]</property>
                <property>/b707/generator/gen-breaker[1]</property>
                <property>/b707/generator/gen-breaker[2]</property>
                <property>/b707/generator/gen-breaker[3]</property>
            </condition>
        </exit>
    </step> 
    <step>
        <message>
            Sincronizar todas as valvulas de alimentacao cruzada ate ao seu encerramento (luzes azuis apagadas) Ligar e desligar   todas as valvulas alguns segundos. 
        </message>
        <view>
                <heading-offset-deg>244.9</heading-offset-deg>
                <pitch-offset-deg>-9.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>31.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.8157</x-m>
                <y-m>0.7496</y-m>
                <z-m>0.9017</z-m>
                <scale>1.8595</scale>
        </marker>
        <error>
            <message>
                Abrir e fechar de valvulas-intercomunicacao - uma vez!
            </message>
            <condition>
                <not><property>/b707/fuel/valves/valve-pos[0]</property></not>
                <not><property>/b707/fuel/valves/valve-pos[1]</property></not>
                <not><property>/b707/fuel/valves/valve-pos[2]</property></not>
                <not><property>/b707/fuel/valves/valve-pos[3]</property></not>
                <not><property>/b707/fuel/valves/valve-pos[4]</property></not>
                <not><property>/b707/fuel/valves/valve-pos[5]</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/fuel/valves/valve-pos[0]</property>
                <property>/b707/fuel/valves/valve-pos[1]</property>
                <property>/b707/fuel/valves/valve-pos[2]</property>
                <property>/b707/fuel/valves/valve-pos[3]</property>
                <property>/b707/fuel/valves/valve-pos[4]</property>
                <property>/b707/fuel/valves/valve-pos[5]</property>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
           Ligar as bombas do alimentador de pressao
        </message>
        <view>
                <heading-offset-deg>244.9</heading-offset-deg>
                <pitch-offset-deg>-9.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>31.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.8074</x-m>
                <y-m>0.7496</y-m>
                <z-m>1.0231</z-m>
                <scale>3.0496</scale>
        </marker>
        <error>
            <message>
                Ligue todas as bombas do alimentador de pressao!
            </message>
            <condition>
                <not><property>/b707/fuel/valves/boost-pump[0]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[1]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[2]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[3]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[4]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[5]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[6]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[7]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[8]</property></not>
                <not><property>/b707/fuel/valves/boost-pump[9]</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/fuel/valves/boost-pump[0]</property>
                <property>/b707/fuel/valves/boost-pump[1]</property>
                <property>/b707/fuel/valves/boost-pump[2]</property>
                <property>/b707/fuel/valves/boost-pump[3]</property>
                <property>/b707/fuel/valves/boost-pump[4]</property>
                <property>/b707/fuel/valves/boost-pump[5]</property>
                <property>/b707/fuel/valves/boost-pump[6]</property>
                <property>/b707/fuel/valves/boost-pump[7]</property>
                <property>/b707/fuel/valves/boost-pump[8]</property>
                <property>/b707/fuel/valves/boost-pump[9]</property>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            Definir todas ENGINE SHUTOFF-VALVE para ON(Ligue TODAS AS VALVULAS DE PARADA DE MOTOR). 
        </message>
        <view>
                <heading-offset-deg>244.9</heading-offset-deg>
                <pitch-offset-deg>-9.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>31.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.8174</x-m>
                <y-m>0.7496</y-m>
                <z-m>1.1000</z-m>
                <scale>3.0496</scale>
        </marker> 
        <error>
            <message>
                TODOS motores SHUTOFF-Valves deve ser definido como ON.
            </message>
            <condition>
                <not><property>/b707/fuel/valves/fuel-shutoff[0]</property></not>
                <not><property>/b707/fuel/valves/fuel-shutoff[1]</property></not>
                <not><property>/b707/fuel/valves/fuel-shutoff[2]</property></not>
                <not><property>/b707/fuel/valves/fuel-shutoff[3]</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/fuel/valves/fuel-shutoff[0]</property>
                <property>/b707/fuel/valves/fuel-shutoff[1]</property>
                <property>/b707/fuel/valves/fuel-shutoff[2]</property>
                <property>/b707/fuel/valves/fuel-shutoff[3]</property>
            </condition>
        </exit>
    </step>       
    <step>
         <message>
          Abra a tampa do acionador de partida 3
         </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <marker>
          <x-m> 0.0322</x-m>
          <y-m> 0.0393</y-m>
          <z-m> 0.1301</z-m>
            <scale>3.0000</scale>
        </marker>
        <exit>
            <condition>
                    <property>/b707/start/startercover[2]</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
        Empurre o acionador de partida 3 e em seguida puxe a alavanca para cortar.
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <marker>
                <x-m>-18.3301</x-m>
                <y-m>0.0149</y-m>
                <z-m>1.4176</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <property>engines/engine[2]/starter</property>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            Levante a alavanca para cortar 3.
        </message>
        <view>
                <heading-offset-deg>300.2</heading-offset-deg>
                <pitch-offset-deg>-38.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>31.1</field-of-view>
        </view>
        <marker>
                <x-m>-18.5140</x-m>
                <y-m>0.0074</y-m>
                <z-m>0.6669</z-m>
                <scale>3.6628</scale>
        </marker>
        <error>
            <message>
                Levante a alavanca 3! (cutoff 3)!
            </message>
            <condition>
                <property>controls/engines/engine[2]/cutoff</property>
            </condition>
        </error>
        <exit>
            <condition>
                <not><property>controls/engines/engine[2]/cutoff</property></not>
            </condition>
        </exit>
    </step>
    <step>
         <message>
         Controle N2 e o outro instrumento para este motor
          </message>
        <view>
                <heading-offset-deg>319.3</heading-offset-deg>
                <pitch-offset-deg>-28.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>52.9</field-of-view>
        </view>
        <marker>
                <x-m>-18.9037</x-m>
                <y-m>-0.0017</y-m>
                <z-m>0.8449</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <greater-than>
                    <property>engines/engine[2]/n2</property>
                    <value>35</value>
                </greater-than>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
        Acionar(Starter) a partida 3 - a luz verde esta apagada?
       </message>
        <view>
                <heading-offset-deg>315.9</heading-offset-deg>
                <pitch-offset-deg>-29.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>39.1</field-of-view>
        </view>
        <marker>
                <x-m>-18.3301</x-m>
                <y-m>0.0149</y-m>
                <z-m>1.4176</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <property>engines/engine[2]/running</property>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
        Feche tampa 3 abra tampa 4
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <exit>
            <condition>
                <property>engines/engine[2]/running</property>
                <property>/b707/start/startercover[3]</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
        Empurre Starter 4 em seguida puxe a alavanca para cortar.
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <marker>
                <x-m>-18.3301</x-m>
                <y-m>0.0719</y-m>
                <z-m>1.4176</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <property>engines/engine[3]/starter</property>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            Levante a alavanca para cortar o 4.
        </message>
        <view>
                <heading-offset-deg>300.2</heading-offset-deg>
                <pitch-offset-deg>-38.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>31.1</field-of-view>
        </view>
 
        <marker>
                <x-m>-18.5140</x-m>
                <y-m>0.0074</y-m>
                <z-m>0.6669</z-m>
                <scale>3.6628</scale>
        </marker>
        <error>
            <message>
                Levante a alavanca 4!
            </message>
            <condition>
                <property>controls/engines/engine[3]/cutoff</property>
            </condition>
        </error>
        <exit>
            <condition>
                <not><property>controls/engines/engine[3]/cutoff</property></not>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
        Verificar N2 e o outro instrumento deste motor
        </message>
        <view>
                <heading-offset-deg>319.3</heading-offset-deg>
                <pitch-offset-deg>-28.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>52.9</field-of-view>
        </view>
        <marker>
                <x-m>-18.9037</x-m>
                <y-m>0.0380</y-m>
                <z-m>0.8449</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <greater-than>
                    <property>engines/engine[3]/n2</property>
                    <value>40</value>
                </greater-than>
            </condition>
        </exit>
    </step> 
    <step>
        <message>
         Acionador de partida 4 - Espere ate a luz verde apagar
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <exit>
            <condition>
                <property>engines/engine[3]/running</property>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
       Abra a tampa 4 feche a tampa 2
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <exit>
            <condition>
                <property>engines/engine[3]/running</property>
                <property>/b707/start/startercover[1]</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
        Acionador de partida 2 em seguida levante a alavanca para cortar.
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <marker>
                <x-m>-18.3301</x-m>
                <y-m>-0.0565</y-m>
                <z-m>1.4102</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <property>engines/engine[1]/starter</property>
            </condition>
        </exit>
    </step>       
    <step>
        <message>
            Suba a alavanca para cortar 2.
        </message>
        <view>
                <heading-offset-deg>300.2</heading-offset-deg>
                <pitch-offset-deg>-38.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>31.1</field-of-view>
        </view>
        <marker>
                <x-m>-18.5140</x-m>
                <y-m>0.0074</y-m>
                <z-m>0.6669</z-m>
                <scale>3.6628</scale>
        </marker>
        <error>
            <message>
                Suba a alavanca 2! 
            </message>
            <condition>
                <property>controls/engines/engine[1]/cutoff</property>
            </condition>
        </error>
        <exit>
            <condition>
                <not><property>controls/engines/engine[1]/cutoff</property></not>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
        Controle N2 e o outro instrumento para este motor
        </message>
        <view>
                <heading-offset-deg>319.3</heading-offset-deg>
                <pitch-offset-deg>-28.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>52.9</field-of-view>
        </view>
        <marker>
                <x-m>-18.9037</x-m>
                <y-m>-0.0430</y-m>
                <z-m>0.8449</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <greater-than>
                    <property>engines/engine[1]/n2</property>
                    <value>40</value>
                </greater-than>
            </condition>
        </exit>
    </step>    
    <step>
        <message>
        Acionador de partida 2 - Espere ate a luz verde apagar
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <exit>
            <condition>
                <property>engines/engine[1]/running</property>
            </condition>
        </exit>
    </step>      
    <step>
        <message>
        Feche a tampa 2 abra tampa 1
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <exit>
            <condition>
                <property>engines/engine[1]/running</property>
                <property>/b707/start/startercover[0]</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
        Acionador de partida 1 e entao levante a alavanca para cortar.
        </message>
        <view>
                <heading-offset-deg>292.9</heading-offset-deg>
                <pitch-offset-deg>27.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>47.4</field-of-view>
        </view>
        <marker>
                <x-m>-18.3301</x-m>
                <y-m>-0.1193</y-m>
                <z-m>1.4102</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <property>engines/engine[0]/starter</property>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            Suba a alavanca para cortar 1.
        </message>
        <view>
                <heading-offset-deg>300.2</heading-offset-deg>
                <pitch-offset-deg>-38.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>31.1</field-of-view>
        </view>
        <marker>
                <x-m>-18.5140</x-m>
                <y-m>0.0074</y-m>
                <z-m>0.6669</z-m>
                <scale>3.6628</scale>
        </marker>
 
        <error>
            <message>
               Suba alavanca para cortar 1!
            </message>
            <condition>
                <property>controls/engines/engine[0]/cutoff</property>
            </condition>
        </error>
        <exit>
            <condition>
                <not><property>controls/engines/engine[0]/cutoff</property></not>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
        Controle N2 e o outro instrumento para este motor
        </message>
        <view>
                <heading-offset-deg>319.3</heading-offset-deg>
                <pitch-offset-deg>-28.3</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.5</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>52.9</field-of-view>
        </view>
        <marker>
                <x-m>-18.9037</x-m>
                <y-m>-0.0843</y-m>
                <z-m>0.8449</z-m>
                <scale>1.9107</scale>
        </marker>
        <exit>
            <condition>
                <greater-than>
                    <property>engines/engine[1]/n2</property>
                    <value>35</value>
                </greater-than>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
        Acionador de partida 1 - Espere ate a luz verde apagar
        </message>
        <view>
            <heading-offset-deg>-75</heading-offset-deg>
            <pitch-offset-deg>30.0</pitch-offset-deg>
            <roll-offset-deg>0.0</roll-offset-deg>
            <x-offset-m>-0.46</x-offset-m>
            <y-offset-m>1.19</y-offset-m>
            <z-offset-m>-18.2</z-offset-m>
            <field-of-view>44.3</field-of-view>
        </view>
        <exit>
            <condition>
                <property>engines/engine[0]/running</property>
            </condition>
        </exit>
    </step>    
    <step>
        <message>
       Feche a tampa 1
       </message>
        <view>
            <heading-offset-deg>-75</heading-offset-deg>
            <pitch-offset-deg>30.0</pitch-offset-deg>
            <roll-offset-deg>0.0</roll-offset-deg>
            <x-offset-m>-0.46</x-offset-m>
            <y-offset-m>1.19</y-offset-m>
            <z-offset-m>-18.2</z-offset-m>
            <field-of-view>44.3</field-of-view>
        </view>
        <exit>
            <condition>
                <not><property>/b707/start/startercover[0]</property></not>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
       Verfique N2 na faixa verde.
        </message>
        <view>
            <heading-offset-deg>-40.0</heading-offset-deg>
            <pitch-offset-deg>-20.0</pitch-offset-deg>
            <roll-offset-deg>0.0</roll-offset-deg>
            <x-offset-m>-0.46</x-offset-m>
            <y-offset-m>1.19</y-offset-m>
            <z-offset-m>-18.2</z-offset-m>
            <field-of-view>44.3</field-of-view>
        </view>
        <exit>
            <condition>
                <greater-than>
                    <property>engines/engine[0]/n2</property>
                    <value>50</value>
                </greater-than>
                <greater-than>
                    <property>engines/engine[1]/n2</property>
                    <value>50</value>
                </greater-than>
                <greater-than>
                    <property>engines/engine[2]/n2</property>
                    <value>50</value>
                </greater-than>
                <greater-than>
                    <property>engines/engine[3]/n2</property>
                    <value>50</value>
                </greater-than>
            </condition>
        </exit>
    </step>      
    <step>
        <message>
            SELETOR AC PARALELO selecione GEN I
            Agora sincronizaremos os geradores.
        </message>
        <view>
                <heading-offset-deg>244.2</heading-offset-deg>
                <pitch-offset-deg>4.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>20.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.6066</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2455</z-m>
                <scale>1.6612</scale>
        </marker>
        <error>
            <message>
            Selecione GEN I
             </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>1</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>1</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ac/ac-para-select</property>
                    <value>1</value>
                </equals>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            Preste atencao a este instrumento durante a sincronizacao
        </message>
        <view>
                <heading-offset-deg>244.2</heading-offset-deg>
                <pitch-offset-deg>4.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>20.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.6182</x-m>
                <y-m>0.6513</y-m>
                <z-m>1.3107</z-m>
                <scale>2.5372</scale>
        </marker>
    </step>
    <step>
        <message>
            Gire o botao de controle de FREQ ate as luzes brancas de controle apagarem.
        </message>
        <view>
                <heading-offset-deg>247.7</heading-offset-deg>
                <pitch-offset-deg>4.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>21.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.8314</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2174</z-m>
                <scale>1.7934</scale>
        </marker>
        <error>
            <message>
            sincronize gerador 1 agora
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/generator/gen-freq[0]</property>
                        <value>400</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/generator/gen-freq[0]</property>
                        <value>400</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/generator/gen-freq[0]</property>
                    <value>400</value>
                </equals>
            </condition>
        </exit>
    </step>
    <step>
        <message>
            Selecione GEN 2 no SELETOR AC PARALELO
        </message>
        <view>
                <heading-offset-deg>244.2</heading-offset-deg>
                <pitch-offset-deg>4.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>20.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.6066</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2455</z-m>
                <scale>1.6612</scale>
        </marker>
        <error>
            <message>
             selecione GEN 2
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>2</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>2</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ac/ac-para-select</property>
                    <value>2</value>
                </equals>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            Gire o botao de controle de FREQ ate as luzes  brancas de controle apagarem
        </message>
        <view>
                <heading-offset-deg>247.7</heading-offset-deg>
                <pitch-offset-deg>4.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>21.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.7785</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2174</z-m>
                <scale>1.7934</scale>
        </marker>
        <error>
            <message>
            sincronize gerador 2 agora
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/generator/gen-freq[1]</property>
                        <value>400</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/generator/gen-freq[1]</property>
                        <value>400</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/generator/gen-freq[1]</property>
                    <value>400</value>
                </equals>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            Selecione GEN 3 no SELECTOR AC PARALELO
        </message>
        <view>
                <heading-offset-deg>244.2</heading-offset-deg>
                <pitch-offset-deg>4.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>20.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.5719</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2695</z-m>
                <scale>1.6612</scale>
        </marker>
        <error>
            <message>
            selecione GEN 3
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>4</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>4</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ac/ac-para-select</property>
                    <value>4</value>
                </equals>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
           Gire o botao de controle de FREQ ate as luzes brancas de controle apagarem
        </message>
        <view>
                <heading-offset-deg>247.7</heading-offset-deg>
                <pitch-offset-deg>4.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>21.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.7248</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2149</z-m>
                <scale>1.7934</scale>
        </marker>
        <error>
            <message>
            sincronize gerador 3 agora
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/generator/gen-freq[2]</property>
                        <value>400</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/generator/gen-freq[2]</property>
                        <value>400</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/generator/gen-freq[2]</property>
                    <value>400</value>
                </equals>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            Selecione GEN 4 no interruptor AC PARALELO
        </message>
        <view>
                <heading-offset-deg>244.2</heading-offset-deg>
                <pitch-offset-deg>4.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>20.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.5719</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2695</z-m>
                <scale>1.6612</scale>
        </marker>
        <error>
            <message>
            Selecione Gen 4
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>5</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>5</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ac/ac-para-select</property>
                    <value>5</value>
                </equals>
            </condition>
        </exit>
    </step> 
    <step>
        <message>
            Gire o botao de controle de FREQ ate as luzes brancas de controle apagarem
        </message>
        <view>
                <heading-offset-deg>247.7</heading-offset-deg>
                <pitch-offset-deg>4.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>21.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.6719</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2149</z-m>
                <scale>1.7934</scale>
        </marker>
        <error>
            <message>
            sincronize gerador 4 agora
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/generator/gen-freq[3]</property>
                        <value>400</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/generator/gen-freq[3]</property>
                        <value>400</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/generator/gen-freq[3]</property>
                    <value>400</value>
                </equals>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            Para controlar, selecione GEN 1 no seletor de AC em paralelo
        </message>
        <view>
                <heading-offset-deg>244.2</heading-offset-deg>
                <pitch-offset-deg>4.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>20.3</field-of-view>
        </view>
        <marker>
                <x-m>-17.6066</x-m>
                <y-m>0.7000</y-m>
                <z-m>1.2455</z-m>
                <scale>1.6612</scale>
        </marker>
        <error>
            <message>
            Selecione GEN 1
             </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>1</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ac/ac-para-select</property>
                        <value>1</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ac/ac-para-select</property>
                    <value>1</value>
                </equals>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            Feche todos os Buses do Regulador Automatico de sincronizacao
        </message>
        <view>
                <heading-offset-deg>244.9</heading-offset-deg>
                <pitch-offset-deg>9.7</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>16.7</field-of-view>
        </view>
        <marker>
                <x-m>-17.8653</x-m>
                <y-m>0.5992</y-m>
                <z-m>1.3669</z-m>
                <scale>1.6628</scale>
        </marker>
        <error>
            <message>
                Feche todos Buses!
            </message>
            <condition>
                <not><property>/b707/generator/gen-bus-tie[0]</property></not>
                <not><property>/b707/generator/gen-bus-tie[1]</property></not>
                <not><property>/b707/generator/gen-bus-tie[2]</property></not>
                <not><property>/b707/generator/gen-bus-tie[3]</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/generator/gen-bus-tie[0]</property>
                <property>/b707/generator/gen-bus-tie[1]</property>
                <property>/b707/generator/gen-bus-tie[2]</property>
                <property>/b707/generator/gen-bus-tie[3]</property>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
           Nossa fonte de energia essencial agora e gerador 1.
           Gire o botao para GEN I
        </message>
        <view>
                <heading-offset-deg>238.1</heading-offset-deg>
                <pitch-offset-deg>7.5</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>14.5</field-of-view>
        </view>
        <marker>
                <x-m>-17.5620</x-m>
                <y-m>0.6000</y-m>
                <z-m>1.3686</z-m>
                <scale>1.3967</scale>
        </marker>
        <error>
            <message>
            Gire para Gerador 1
            </message>
            <condition>
                <or>
                    <less-than>
                        <property>/b707/ess-power-switch</property>
                        <value>1</value>
                    </less-than>
                    <greater-than>
                        <property>/b707/ess-power-switch</property>
                        <value>1</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <equals>
                    <property>/b707/ess-power-switch</property>
                    <value>1</value>
                </equals>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
            Cortar a ligacao com a unidade de potencia
        </message>
        <view>
                <heading-offset-deg>237.8</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.3</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>15.9</field-of-view>
        </view>
        <marker>
                <x-m>-17.5785</x-m>
                <y-m>0.6000</y-m>
                <z-m>1.4091</z-m>
                <scale>1.4959</scale>
        </marker>
        <error>
            <message>
                selecione OFF para cortar.
            </message>
            <condition>
                <property>/b707/ground-connect</property>
            </condition>
        </error>
        <exit>
            <condition>
                <not><property>/b707/ground-connect</property></not>
            </condition>
        </exit>
    </step>
    <step>
        <message>
         Desconecte da fonte de alimentacao externa 
         Selecione no menu principal - Boeing 707/ unidade de Potencia Externa
        </message>
        <view>
                <heading-offset-deg>240.8</heading-offset-deg>
                <pitch-offset-deg>4.0</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>49.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.5636</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.3967</z-m>
                <scale>1.6612</scale>
        </marker>
        <exit>
            <condition>
                <not><property>/b707/external-power-connected</property></not>
            </condition>
        </exit>
    </step>   
    <step>
        <message>
           Unidade de alimentacao externa e desligado
        </message>
        <view>
            <view-number>1</view-number>
            <heading-offset-deg>182.1</heading-offset-deg>
            <pitch-offset-deg>-4.6</pitch-offset-deg>
            <roll-offset-deg>0.0</roll-offset-deg>
            <x-offset-m>0.3</x-offset-m>
            <y-offset-m>1.8</y-offset-m>
            <z-offset-m>-32.0</z-offset-m>
            <field-of-view>70</field-of-view>
        </view>
        <exit>
            <condition>
                <not><property>/b707/external-power-connected</property></not>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            Conversor de 40 Hertz - controla 115 volts 60 ciclo de forca para o camarote e as areas de cozinha numero dois.
        </message>
        <view>
            <heading-offset-deg>239.9</heading-offset-deg>
            <pitch-offset-deg>-4.9</pitch-offset-deg>
            <roll-offset-deg>0.0</roll-offset-deg>
            <x-offset-m>-0.4</x-offset-m>
            <y-offset-m>1.2</y-offset-m>
            <z-offset-m>-18.2</z-offset-m>
            <field-of-view>28.6</field-of-view>
        </view>
        <marker>
            <x-m>-17.5876</x-m>
            <y-m>0.5711</y-m>
            <z-m>1.0636</z-m>
            <scale>1.6612</scale>
        </marker>
        <error>
            <message>
               Interruptor para ON.
            </message>
            <condition>
                <not><property>/b707/generator/hertz-converter</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/generator/hertz-converter</property>
            </condition>
        </exit>
    </step>   
    <step>
        <message>       	
        Definir bombas de refrigeracao para ON.
        </message>
        <view>
                <heading-offset-deg>239.9</heading-offset-deg>
                <pitch-offset-deg>-4.9</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>28.6</field-of-view>
        </view>
        <marker>
                <x-m>-17.5876</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.1157</z-m>
                <scale>1.6612</scale>
        </marker>
        <error>
            <message>
                Ooloque interruptores para ON.
            </message>
            <condition>
                <not><property>/b707/equipment/ovbd-dump</property></not>
                <not><property>/b707/equipment/blower</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/equipment/ovbd-dump</property>
                <property>/b707/equipment/blower</property>
            </condition>
        </exit>
    </step>  
    <step>
        <message>
            Abra a tampa para RAM Air e ligue-a.
        </message>
        <view>
                <heading-offset-deg>229.9</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>30.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.3264</x-m>
                <y-m>0.5356</y-m>
                <z-m>1.4959</z-m>
                <scale>2.3224</scale>
        </marker>
        <error>
            <message>
               Setar o interruptor para Open.
            </message>
            <condition>
                <not><property>/b707/air-conditioning/ram-air-switch</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/air-conditioning/ram-air-switch</property>
            </condition>
        </exit>
    </step>    
    <step>
        <message>
            Ligar Compressor de Ar no motor 2.
        </message>
        <view>
                <heading-offset-deg>229.9</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>30.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.5041</x-m>
                <y-m>0.5356</y-m>
                <z-m>1.4579</z-m>
                <scale>2.3224</scale>
        </marker>
        <error>
            <message>
               Coloque em START. Se a RPM exceder 115% reinicie o compressor.
            </message>
            <condition>
                <not><property>/b707/air-conditioning/compressor-start[0]</property></not>
                <greater-than>
                    <property>/b707/air-conditioning/compressor-rpm[0]</property>
                    <value>115</value>
                </greater-than>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/air-conditioning/compressor-start[0]</property>
                <less-than>
                    <property>/b707/air-conditioning/compressor-rpm[0]</property>
                    <value>115</value>
                </less-than>
                <greater-than>
                    <property>/b707/air-conditioning/compressor-rpm[0]</property>
                    <value>90</value>
                </greater-than>    
            </condition>
        </exit>
    </step>     
    <step>
        <message>
           Ligar Compressor de Ar no motor 3.
        </message>
        <view>
                <heading-offset-deg>229.9</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>30.1</field-of-view>
        </view> 
        <marker>
                <x-m>-17.4537</x-m>
                <y-m>0.5356</y-m>
                <z-m>1.4579</z-m>
                <scale>2.3224</scale>
        </marker>
        <error>
            <message>
                Coloca-lo na posicao START. Se RPM exceder 115% reiniciar o compressor.
                Veja tambem a luz ambar de compressor 1. Se for necessario reiniciar o primeiro.
            </message>
            <condition>
                <not><property>/b707/air-conditioning/compressor-start[1]</property></not>
                <or>            
                    <greater-than>
                        <property>/b707/air-conditioning/compressor-rpm[1]</property>
                        <value>115</value>
                    </greater-than>                
                    <greater-than>
                        <property>/b707/air-conditioning/compressor-rpm[0]</property>
                        <value>115</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/air-conditioning/compressor-start[1]</property>
                <less-than>
                    <property>/b707/air-conditioning/compressor-rpm[1]</property>
                    <value>115</value>
                </less-than>
                <greater-than>
                    <property>/b707/air-conditioning/compressor-rpm[1]</property>
                    <value>90</value>
                </greater-than>    
            </condition>
        </exit>
    </step>
    <step>
        <message>
            Ligue Compressor de Ar motor 4.
        </message>
        <view>
                <heading-offset-deg>229.9</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>30.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.4041</x-m>
                <y-m>0.5356</y-m>
                <z-m>1.4579</z-m>
                <scale>2.3224</scale>
        </marker>
        <error>
            <message>
                Alternar para iniciar. Se o RPM exceder 115% reinicie o compressor.
                Veja tambem a luz ambar dos compressores 1 e 2. Reinicie-os se necessario.
            </message>
            <condition>
                <not><property>/b707/air-conditioning/compressor-start[2]</property></not>
                <or>
                    <greater-than>
                        <property>/b707/air-conditioning/compressor-rpm[2]</property>
                        <value>115</value>
                    </greater-than>                
                    <greater-than>
                        <property>/b707/air-conditioning/compressor-rpm[1]</property>
                        <value>115</value>
                    </greater-than>                
                    <greater-than>
                        <property>/b707/air-conditioning/compressor-rpm[0]</property>
                        <value>115</value>
                    </greater-than>
                </or>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/air-conditioning/compressor-start[2]</property>
                <less-than>
                    <property>/b707/air-conditioning/compressor-rpm[2]</property>
                    <value>115</value>
                </less-than>
                <greater-than>
                    <property>/b707/air-conditioning/compressor-rpm[2]</property>
                    <value>90</value>
                </greater-than>    
            </condition>
        </exit>
    </step>
    <step>
        <message>
            Conecte as valvulas de borboleta.
        </message>
        <view>
                <heading-offset-deg>229.9</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>30.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.4801</x-m>
                <y-m>0.5356</y-m>
                <z-m>1.4166</z-m>
                <scale>2.3224</scale>
        </marker>
        <error>
            <message>
               Abra o conduto cruzado L e R para ABRIR.
            </message>
            <condition>
                <not><property>/b707/air-conditioning/wing-valve[0]</property></not>
                <not><property>/b707/air-conditioning/wing-valve[1]</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/air-conditioning/wing-valve[0]</property>
                <property>/b707/air-conditioning/wing-valve[1]</property>
            </condition>
        </exit>
    </step>
    <step>
        <message>
            Abra os interruptores da unidade de ar condicionado. Primeiro abra a tampa.
        </message>
        <view>
                <heading-offset-deg>229.9</heading-offset-deg>
                <pitch-offset-deg>8.2</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>30.1</field-of-view>
        </view>
        <marker>
                <x-m>-17.4933</x-m>
                <y-m>0.5356</y-m>
                <z-m>1.3620</z-m>
                <scale>3.2811</scale>
        </marker>
        <error>
            <message>
             Abra as unidades de ar condicionado. Defina-a como ON.
            </message>
            <condition>
                <not><property>/b707/air-conditioning/air-cond-unit-left-start</property></not>
                <not><property>/b707/air-conditioning/air-cond-unit-right-start</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/air-conditioning/air-cond-unit-left-start</property>
                <property>/b707/air-conditioning/air-cond-unit-right-start</property>
            </condition>
        </exit>
    </step>    
    <step>
        <message>
            Abra a tampa da valvula de seguranca-ar.(Safety-Air-valve.)
            Mude o botao para baixo.
        </message>
        <view>
                <heading-offset-deg>227.6</heading-offset-deg>
                <pitch-offset-deg>3.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>23.5</field-of-view>
        </view>
        <marker>
                <x-m>-17.1619</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.3967</z-m>
                <scale>2.3224</scale>
        </marker>
        <error>
            <message>
               Alternar para baixo o botao, a luz ambar apagara.
            </message>
            <condition>
                <not><property>/b707/pressurization/safety-valve</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/pressurization/safety-valve</property>
            </condition>
        </exit>
    </step>          
    <step>
        <message>
            Agora ligue o modo automatico de pressurizacao.
        </message>
        <view>
                <heading-offset-deg>227.6</heading-offset-deg>
                <pitch-offset-deg>3.8</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>23.5</field-of-view>
        </view>
        <marker>
                <x-m>-17.4264</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.2380</z-m>
                <scale>1.8100</scale>
        </marker>
        <error>
            <message>
                Setar o interruptor para ON.
            </message>
            <condition>
                <not><property>/b707/pressurization/manual-mode-switch</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/pressurization/manual-mode-switch</property>
            </condition>
        </exit>
    </step>    
    <step>
        <message>
            Selecione posicao decolagem(takeoff). 
        </message>
        <view>
                <heading-offset-deg>235.3</heading-offset-deg>
                <pitch-offset-deg>1.4</pitch-offset-deg>
                <roll-offset-deg>0.0</roll-offset-deg>
                <x-offset-m>-0.4</x-offset-m>
                <y-offset-m>1.2</y-offset-m>
                <z-offset-m>-18.2</z-offset-m>
                <field-of-view>14.3</field-of-view>
        </view> 
        <marker>
                <x-m>-17.5785</x-m>
                <y-m>0.5711</y-m>
                <z-m>1.2380</z-m>
                <scale>1.1488</scale>
        </marker>
        <error>
            <message>
                Setar o interruptor para ON.
            </message>
            <condition>
                <not><property>/b707/pressurization/mode-switch</property></not>
            </condition>
        </error>
        <exit>
            <condition>
                <property>/b707/pressurization/mode-switch</property>
            </condition>
        </exit>
    </step>               
    <end>
        <message>
         Todos os motores comecaram. Geradores fechados. Tenha um bom Voo!
        </message>
        <view>
            <heading-offset-deg>0</heading-offset-deg>
            <pitch-offset-deg>-16</pitch-offset-deg>
            <field-of-view>72</field-of-view>
        </view>
    </end>
 
</PropertyList>